#
# Copyright 2012 Jared Boone
#
# This file is part of HackRF.
#
# This program is free software; you can redistribute it and/or modify
# it under the terms of the GNU General Public License as published by
# the Free Software Foundation; either version 2, or (at your option)
# any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; see the file COPYING.  If not, write to
# the Free Software Foundation, Inc., 51 Franklin Street,
# Boston, MA 02110-1301, USA.

NET "CODEC_CLK"    LOC="23" |FAST |IOSTANDARD=LVCMOS18;
NET "CODEC_X2_CLK" LOC="27" |FAST |IOSTANDARD=LVCMOS18;
#NET "GCLK0" LOC="22" |FAST |IOSTANDARD=LVCMOS18;

NET "CODEC_X2_CLK" TNM_NET = CODEC_X2_CLK;
TIMESPEC TS_codec_x2_data = PERIOD "CODEC_X2_CLK" 50 ns;

NET "DA<7>" LOC="35" |FAST |IOSTANDARD=LVCMOS18;
NET "DA<6>" LOC="36" |FAST |IOSTANDARD=LVCMOS18;
NET "DA<5>" LOC="37" |FAST |IOSTANDARD=LVCMOS18;
NET "DA<4>" LOC="39" |FAST |IOSTANDARD=LVCMOS18;
NET "DA<3>" LOC="40" |FAST |IOSTANDARD=LVCMOS18;
NET "DA<2>" LOC="41" |FAST |IOSTANDARD=LVCMOS18;
NET "DA<1>" LOC="42" |FAST |IOSTANDARD=LVCMOS18;
NET "DA<0>" LOC="43" |FAST |IOSTANDARD=LVCMOS18;

NET "DD<9>" LOC="17" |FAST |IOSTANDARD=LVCMOS18;
NET "DD<8>" LOC="18" |FAST |IOSTANDARD=LVCMOS18;
NET "DD<7>" LOC="19" |FAST |IOSTANDARD=LVCMOS18;
NET "DD<6>" LOC="24" |FAST |IOSTANDARD=LVCMOS18;
NET "DD<5>" LOC="28" |FAST |IOSTANDARD=LVCMOS18;
NET "DD<4>" LOC="29" |FAST |IOSTANDARD=LVCMOS18;
NET "DD<3>" LOC="30" |FAST |IOSTANDARD=LVCMOS18;
NET "DD<2>" LOC="32" |FAST |IOSTANDARD=LVCMOS18;
NET "DD<1>" LOC="33" |FAST |IOSTANDARD=LVCMOS18;
NET "DD<0>" LOC="34" |FAST |IOSTANDARD=LVCMOS18;

NET "B1AUX<16>" LOC="60" |FAST |IOSTANDARD=LVCMOS18;
NET "B1AUX<15>" LOC="58" |FAST |IOSTANDARD=LVCMOS18;
NET "B1AUX<14>" LOC="56" |FAST |IOSTANDARD=LVCMOS18;
NET "B1AUX<13>" LOC="55" |FAST |IOSTANDARD=LVCMOS18;
NET "B1AUX<12>" LOC="53" |FAST |IOSTANDARD=LVCMOS18;
NET "B1AUX<11>" LOC="52" |FAST |IOSTANDARD=LVCMOS18;
NET "B1AUX<10>" LOC="50" |FAST |IOSTANDARD=LVCMOS18;
NET "B1AUX<9>"  LOC="49" |FAST |IOSTANDARD=LVCMOS18;

NET "SGPIO<15>" LOC="78" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<14>" LOC="81" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<13>" LOC="90" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<12>" LOC="70" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<11>" LOC="71" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<10>" LOC="76" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<9>"  LOC="91" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<8>"  LOC="68" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<7>"  LOC="77" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<6>"  LOC="61" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<5>"  LOC="64" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<4>"  LOC="67" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<3>"  LOC="72" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<2>"  LOC="74" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<1>"  LOC="79" |FAST |IOSTANDARD=LVCMOS33;
NET "SGPIO<0>"  LOC="89" |FAST |IOSTANDARD=LVCMOS33;

NET "B2AUX<16>" LOC="92" |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<15>" LOC="94" |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<14>" LOC="97" |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<13>" LOC="99" |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<12>" LOC="1"  |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<11>" LOC="2"  |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<10>" LOC="3"  |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<9>"  LOC="4"  |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<8>"  LOC="6"  |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<7>"  LOC="7"  |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<6>"  LOC="8"  |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<5>"  LOC="9"  |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<4>"  LOC="10" |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<3>"  LOC="11" |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<2>"  LOC="12" |FAST |IOSTANDARD=LVCMOS33;
NET "B2AUX<1>"  LOC="13" |FAST |IOSTANDARD=LVCMOS33;
