(export (version D)
  (design
    (source /home/mossmann/src/hackrf/hardware/LNA915/LNA915.sch)
    (date "Sun Feb  9 14:18:41 2014")
    (tool "eeschema (2013-07-24 BZR 4024)-stable"))
  (components
    (comp (ref D3)
      (value PIN)
      (fields
        (field (name Manufacturer) NXP)
        (field (name "Part Number") BAP50-03)
        (field (name Description) "DIODE PIN GP 50V 100MA SOD323"))
      (libsource (lib device) (part DIODE))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F440C5))
    (comp (ref P1)
      (value HACKRF)
      (fields
        (field (name Manufacturer) "Linx Technology")
        (field (name "Part Number") CONSMA003.062)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F440F7))
    (comp (ref D1)
      (value GSG-DIODE-TVS-BI)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-100)
        (field (name Description) "TVS DIODE ESD .05PF 15KV 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F44107))
    (comp (ref C5)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F44170))
    (comp (ref U2)
      (value SAW)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") FAR-F5QA-915M00-M2AK-J)
        (field (name Description) "FILTER SAW 915MHZ ISM900 SMD"))
      (libsource (lib hackrf) (part FAR-F5QA))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F44412))
    (comp (ref D4)
      (value LNALED)
      (fields
        (field (name Manufacturer) Everlight)
        (field (name "Part Number") QTLP601C4TR)
        (field (name Description) "LED GREEN STD BRIGHT 0603 SMD"))
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F51772))
    (comp (ref U3)
      (value LNA)
      (fields
        (field (name Manufacturer) Infineon)
        (field (name "Part Number") "BGB 741L7ESD E6327")
        (field (name Description) "IC AMP MMIC LNA TSLP7-1"))
      (libsource (lib hackrf) (part BGB741L7ESD))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F68792))
    (comp (ref R6)
      (value 3k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402FT3K00)
        (field (name Description) "RES 3K OHM 1/16W 1% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F68800))
    (comp (ref L5)
      (value 39nH)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") HK100539NJ-T)
        (field (name Description) "INDUCTOR HI FREQ 39NH 5% 0402"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F688CD))
    (comp (ref C10)
      (value 1uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ105KV-F)
        (field (name Description) "CAP CER 1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F68A00))
    (comp (ref L3)
      (value 39nH)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") HK100539NJ-T)
        (field (name Description) "INDUCTOR HI FREQ 39NH 5% 0402"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F68C24))
    (comp (ref L1)
      (value 39nH)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") HK100539NJ-T)
        (field (name Description) "INDUCTOR HI FREQ 39NH 5% 0402"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F68C64))
    (comp (ref R7)
      (value 470)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F68CBB))
    (comp (ref U1)
      (value SWITCH)
      (fields
        (field (name Manufacturer) NXP)
        (field (name "Part Number") BF1118,215)
        (field (name Description) "IC RF SWITCH SOT143B"))
      (libsource (lib hackrf) (part BF1118))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F68FC4))
    (comp (ref R1)
      (value 47k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT47K0)
        (field (name Description) "RES 47K OHM 1/16W 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F6905B))
    (comp (ref R3)
      (value 4k7)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT4K70)
        (field (name Description) "RES 4.7K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F6921D))
    (comp (ref R4)
      (value 100k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT100K)
        (field (name Description) "RES 100K OHM 1/16W 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F69223))
    (comp (ref L4)
      (value 39nH)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") HK100539NJ-T)
        (field (name Description) "INDUCTOR HI FREQ 39NH 5% 0402"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F6975B))
    (comp (ref L2)
      (value 39nH)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") HK100539NJ-T)
        (field (name Description) "INDUCTOR HI FREQ 39NH 5% 0402"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F69884))
    (comp (ref C6)
      (value 1nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71H102KA01D)
        (field (name Description) "CAP CER 1000PF 50V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F69BA3))
    (comp (ref C7)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F69E98))
    (comp (ref C8)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F69EB1))
    (comp (ref C9)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F69EBA))
    (comp (ref C2)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F69EC3))
    (comp (ref C1)
      (value 100pF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F69ECC))
    (comp (ref C11)
      (value 1uF)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ105KV-F)
        (field (name Description) "CAP CER 1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F69F2A))
    (comp (ref D2)
      (value GSG-DIODE-TVS-BI)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-100)
        (field (name Description) "TVS DIODE ESD .05PF 15KV 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F69FCE))
    (comp (ref P2)
      (value ANTENNA)
      (fields
        (field (name Manufacturer) "Linx Technology")
        (field (name "Part Number") CONSMA003.062)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F6A116))
    (comp (ref R5)
      (value 470)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F6A21F))
    (comp (ref C4)
      (value 1nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71H102KA01D)
        (field (name Description) "CAP CER 1000PF 50V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F6A3F1))
    (comp (ref C3)
      (value 1nF)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71H102KA01D)
        (field (name Description) "CAP CER 1000PF 50V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F6A40A))
    (comp (ref R2)
      (value 100k)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT100K)
        (field (name Description) "RES 100K OHM 1/16W 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F6A598))
    (comp (ref P3)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F7A9D0))
    (comp (ref P4)
      (value CONN_1)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 52F7A9E7)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part DIODE)
      (description "Diode simple")
      (footprints
        (fp D?)
        (fp S*))
      (fields
        (field (name Reference) D)
        (field (name Value) DIODE))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part INDUCTOR)
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_1)
      (description "1 pin")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib hackrf) (part BF1118)
      (fields
        (field (name Reference) U)
        (field (name Value) BF1118)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name K) (type power_in))
        (pin (num 3) (name S) (type BiDi))
        (pin (num 4) (name D) (type BiDi))))
    (libpart (lib hackrf) (part BGB741L7ESD)
      (fields
        (field (name Reference) U)
        (field (name Value) BGB741L7ESD)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VCC) (type power_in))
        (pin (num 2) (name BIAS) (type output))
        (pin (num 3) (name RFIN) (type input))
        (pin (num 4) (name RFOUT) (type output))
        (pin (num 5) (name VCTRL) (type input))
        (pin (num 6) (name ADJ) (type input))
        (pin (num 7) (name GND) (type power_in))))
    (libpart (lib hackrf) (part FAR-F5QA)
      (fields
        (field (name Reference) U)
        (field (name Value) FAR-F5QA)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name IN) (type BiDi))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name OUT) (type BiDi))
        (pin (num 5) (name GND) (type power_in))))
    (libpart (lib hackrf) (part GSG-DIODE-TVS-BI)
      (description "Diode zener")
      (footprints
        (fp D?)
        (fp SO*)
        (fp SM*))
      (fields
        (field (name Reference) D)
        (field (name Value) GSG-DIODE-TVS-BI)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib hackrf) (part GSG-RF-CONN)
      (fields
        (field (name Reference) P)
        (field (name Value) GSG-RF-CONN)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name RF) (type BiDi))
        (pin (num 2) (name GND) (type power_in)))))
  (libraries
    (library (logical device)
      (uri /usr/local/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/local/share/kicad/library/conn.lib))
    (library (logical hackrf)
      (uri ../kicad/hackrf.lib)))
  (nets
    (net (code 1) (name VCC)
      (node (ref R1) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref L1) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref U3) (pin 5))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref L5) (pin 1))
      (node (ref R6) (pin 1)))
    (net (code 2) (name "")
      (node (ref C8) (pin 1))
      (node (ref D3) (pin 2))
      (node (ref L4) (pin 2)))
    (net (code 3) (name GND)
      (node (ref U2) (pin 5))
      (node (ref U2) (pin 3))
      (node (ref U3) (pin 7))
      (node (ref D4) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref C10) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref P1) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref L4) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref P4) (pin 1))
      (node (ref P3) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref P2) (pin 2))
      (node (ref C11) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 4) (name "")
      (node (ref U1) (pin 3))
      (node (ref C1) (pin 2)))
    (net (code 5) (name "")
      (node (ref U1) (pin 4))
      (node (ref C2) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 6) (name "")
      (node (ref L2) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref D3) (pin 1)))
    (net (code 7) (name "")
      (node (ref U1) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 8) (name "")
      (node (ref P2) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 9) (name "")
      (node (ref R7) (pin 2))
      (node (ref D4) (pin 1)))
    (net (code 10) (name "")
      (node (ref U2) (pin 4))
      (node (ref C1) (pin 1))
      (node (ref C7) (pin 1)))
    (net (code 11) (name "")
      (node (ref L2) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref R5) (pin 2)))
    (net (code 12) (name "")
      (node (ref C5) (pin 2))
      (node (ref U2) (pin 1)))
    (net (code 13) (name "")
      (node (ref R6) (pin 2))
      (node (ref U3) (pin 6)))
    (net (code 14) (name "")
      (node (ref C9) (pin 2))
      (node (ref P1) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref L1) (pin 1))
      (node (ref C2) (pin 2)))
    (net (code 15) (name "")
      (node (ref L5) (pin 2))
      (node (ref C9) (pin 1))
      (node (ref U3) (pin 4)))
    (net (code 16) (name "")
      (node (ref L3) (pin 1))
      (node (ref U3) (pin 3))
      (node (ref C8) (pin 2)))
    (net (code 17) (name "")
      (node (ref U3) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref L3) (pin 2)))))