(export (version D)
  (design
    (source /home/mossmann/src/hackrf/hardware/neapolitan/neapolitan.sch)
    (date "Wed 21 Sep 2016 04:41:20 PM MDT")
    (tool "Eeschema (2015-08-18 BZR 6102)-product")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title Neapolitan)
        (company "Copyright 2012 - 2016 Great Scott Gadgets")
        (rev)
        (date "13 feb 2014")
        (source neapolitan.sch)
        (comment (number 1) (value "License: GPL v2"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /frontend/) (tstamps /503BB638/)
      (title_block
        (title "Neapolitan frontend")
        (company "Copyright 2012 - 2016 Great Scott Gadgets")
        (rev)
        (date "13 feb 2014")
        (source frontend.sch)
        (comment (number 1) (value "License: GPL v2"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /baseband/) (tstamps /50370666/)
      (title_block
        (title "Neapolitan baseband")
        (company "Copyright 2012 - 2016 Great Scott Gadgets")
        (rev)
        (date "13 feb 2014")
        (source baseband.sch)
        (comment (number 1) (value "License: GPL v2"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /mcu/usb/power/) (tstamps /5037043E/)
      (title_block
        (title "Neapolitan mcu/usb/power")
        (company "Copyright 2012 - 2016 Great Scott Gadgets")
        (rev)
        (date "13 feb 2014")
        (source mcu.sch)
        (comment (number 1) (value "License: GPL v2"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C53)
      (value 1uF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ105KV-F)
        (field (name Description) "CAP CER 1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 5054932E))
    (comp (ref R24)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503C490B))
    (comp (ref R29)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503C48ED))
    (comp (ref U25)
      (value MGA-81563)
      (footprint hackrf:GSG-SOT363)
      (fields
        (field (name Manufacturer) Avago)
        (field (name "Part Number") MGA-81563-TR1G)
        (field (name Description) "0.1-6 GHz 3 V, 14 dBm Amplifier"))
      (libsource (lib hackrf) (part MGA-81563))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2DD))
    (comp (ref L12)
      (value 10uH)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T100M)
        (field (name Description) "INDUCTR 10UH 220MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2DC))
    (comp (ref C160)
      (value 100pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2DB))
    (comp (ref C161)
      (value 1uF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ105KV-F)
        (field (name Description) "CAP CER 1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2DA))
    (comp (ref Q2)
      (value MOSFET_P)
      (footprint gsg-modules:SOT23GDS)
      (fields
        (field (name Manufacturer) Fairchild)
        (field (name "Part Number") BSS84)
        (field (name Description) "MOSFET P-CH 50V 130MA SOT-23"))
      (libsource (lib neapolitan-cache) (part MOSFET_P))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2D7))
    (comp (ref C162)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2D5))
    (comp (ref C163)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2CB))
    (comp (ref L3)
      (value 10uH)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T100M)
        (field (name Description) "INDUCTR 10UH 220MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2B7))
    (comp (ref L2)
      (value 10uH)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T100M)
        (field (name Description) "INDUCTR 10UH 220MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BF2A7))
    (comp (ref C49)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BB2CE))
    (comp (ref C25)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 503BB2BD))
    (comp (ref C57)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E7A16))
    (comp (ref C55)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E7A10))
    (comp (ref C60)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E79FA))
    (comp (ref C63)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E79CE))
    (comp (ref C66)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E798C))
    (comp (ref C65)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E7989))
    (comp (ref C38)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E792B))
    (comp (ref C40)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E7922))
    (comp (ref C39)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E78E2))
    (comp (ref C29)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6FEE))
    (comp (ref C19)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6F8B))
    (comp (ref C24)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6F11))
    (comp (ref C10)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6EFB))
    (comp (ref C45)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6ECB))
    (comp (ref C54)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6EB0))
    (comp (ref Q1)
      (value MOSFET_P)
      (footprint gsg-modules:SOT23GDS)
      (fields
        (field (name Manufacturer) Fairchild)
        (field (name "Part Number") BSS84)
        (field (name Description) "MOSFET P-CH 50V 130MA SOT-23"))
      (libsource (lib neapolitan-cache) (part MOSFET_P))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E69D1))
    (comp (ref C61)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502E6909))
    (comp (ref U13)
      (value MGA-81563)
      (footprint hackrf:GSG-SOT363)
      (fields
        (field (name Manufacturer) Avago)
        (field (name "Part Number") MGA-81563-TR1G)
        (field (name Description) "0.1-6 GHz 3 V, 14 dBm Amplifier"))
      (libsource (lib hackrf) (part MGA-81563))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502DE480))
    (comp (ref C64)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502C6D4A))
    (comp (ref C52)
      (value 100pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502C6D36))
    (comp (ref L5)
      (value 10uH)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T100M)
        (field (name Description) "INDUCTR 10UH 220MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502C6D12))
    (comp (ref U14)
      (value SKY13317)
      (footprint hackrf:GSG-SKY13317-373LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13317-373LF)
        (field (name Description) "20 MHz-6.0 GHz pHEMT GaAs SP3T Switch"))
      (libsource (lib hackrf) (part SKY13317))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502C6BE2))
    (comp (ref U12)
      (value SKY13317)
      (footprint hackrf:GSG-SKY13317-373LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13317-373LF)
        (field (name Description) "20 MHz-6.0 GHz pHEMT GaAs SP3T Switch"))
      (libsource (lib hackrf) (part SKY13317))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502C6BDF))
    (comp (ref U4)
      (value RFFC5072)
      (footprint hackrf:GSG-QFN32)
      (fields
        (field (name Manufacturer) RFMD)
        (field (name "Part Number") RFFC5072TR7)
        (field (name Description) "WIDEBAND SYNTHESIZER/VCO WITH INTEGRATED 6GHz MIXER"))
      (libsource (lib hackrf) (part RFFC5072))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502BE21C))
    (comp (ref C43)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B5738))
    (comp (ref C32)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B571F))
    (comp (ref U9)
      (value SKY13317)
      (footprint hackrf:GSG-SKY13317-373LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13317-373LF)
        (field (name Description) "20 MHz-6.0 GHz pHEMT GaAs SP3T Switch"))
      (libsource (lib hackrf) (part SKY13317))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B5704))
    (comp (ref C31)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B56C2))
    (comp (ref C9)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B53A4))
    (comp (ref C48)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF6BA))
    (comp (ref C23)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B4C6F))
    (comp (ref U10)
      (value SKY13350)
      (footprint hackrf:GSG-SKY13350-385LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B4C1C))
    (comp (ref C46)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B4C15))
    (comp (ref L4)
      (value DNP)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FB55E30))
    (comp (ref U2)
      (value SKY13350)
      (footprint hackrf:GSG-SKY13350-385LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B490F))
    (comp (ref C33)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B4780))
    (comp (ref U7)
      (value SKY13350)
      (footprint hackrf:GSG-SKY13350-385LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B477E))
    (comp (ref C28)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B477A))
    (comp (ref C22)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502B4779))
    (comp (ref L1)
      (value DNP)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 502AFA8C))
    (comp (ref C16)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F4793))
    (comp (ref C7)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F4788))
    (comp (ref C47)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F477D))
    (comp (ref C56)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F4769))
    (comp (ref C11)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F46A8))
    (comp (ref C20)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F41BD))
    (comp (ref C17)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F41BB))
    (comp (ref C18)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F41B9))
    (comp (ref C44)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F4169))
    (comp (ref U5)
      (value SKY13350)
      (footprint hackrf:GSG-SKY13350-385LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501F3B20))
    (comp (ref C8)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF782))
    (comp (ref U1)
      (value SKY13350)
      (footprint hackrf:GSG-SKY13350-385LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF778))
    (comp (ref C21)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF768))
    (comp (ref C51)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF6A1))
    (comp (ref U11)
      (value SKY13350)
      (footprint hackrf:GSG-SKY13350-385LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF646))
    (comp (ref T2)
      (value MIX_OUT_BALUN)
      (footprint hackrf:GSG-B0310J50100AHF)
      (fields
        (field (name Manufacturer) Anaren)
        (field (name "Part Number") B0310J50100AHF)
        (field (name Description) "Ultra Low Profile 0805 Balun 50 to 100 ohm Balanced"))
      (libsource (lib hackrf) (part BALUN-B0310J50100AHF))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF4A4))
    (comp (ref T1)
      (value MIX_IN_BALUN)
      (footprint hackrf:GSG-B0310J50100AHF)
      (fields
        (field (name Manufacturer) Anaren)
        (field (name "Part Number") B0310J50100AHF)
        (field (name Description) "Ultra Low Profile 0805 Balun 50 to 100 ohm Balanced"))
      (libsource (lib hackrf) (part BALUN-B0310J50100AHF))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF483))
    (comp (ref C27)
      (value 47pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JA01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF311))
    (comp (ref U6)
      (value SKY13350)
      (footprint hackrf:GSG-SKY13350-385LF)
      (fields
        (field (name Manufacturer) Skyworks)
        (field (name "Part Number") SKY13350-385LF)
        (field (name Description) "0.01-6.0 GHz GaAs SPDT Switch"))
      (libsource (lib hackrf) (part SKY13350))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 501EF258))
    (comp (ref C41)
      (value 100pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FB55FAD))
    (comp (ref D1)
      (value GSG-DIODE-TVS-BI)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") LXES15AAA1-100)
        (field (name Description) "TVS DIODE ESD .05PF 15KV 0402"))
      (libsource (lib hackrf) (part GSG-DIODE-TVS-BI))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FB3F9B0))
    (comp (ref R6)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECFAE))
    (comp (ref C37)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECE75))
    (comp (ref C36)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECE73))
    (comp (ref C35)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECE70))
    (comp (ref C34)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECE69))
    (comp (ref R5)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECE50))
    (comp (ref R4)
      (value 51k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402FT51K0)
        (field (name Description) "RES TF 51K OHM 1% 0.0625W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECC79))
    (comp (ref C6)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECBBA))
    (comp (ref C5)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECBB9))
    (comp (ref C3)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECBB6))
    (comp (ref C4)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECBB5))
    (comp (ref C2)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECBA0))
    (comp (ref C1)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAECB99))
    (comp (ref R3)
      (value 22k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Panasonic)
        (field (name "Part Number") ERJ-2GEJ223X)
        (field (name Description) "RES 22K OHM 1/10W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC8B2))
    (comp (ref C15)
      (value 180pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H181JA01D)
        (field (name Description) "CAP CER 180PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC8B0))
    (comp (ref C14)
      (value 8p2)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") UMK105CG8R2DV-F)
        (field (name Description) "CAP CER 8.2PF 50V NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC8AD))
    (comp (ref R2)
      (value 470)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC856))
    (comp (ref C13)
      (value 330pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71H331KA01D)
        (field (name Description) "CAP CER 330PF 50V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC853))
    (comp (ref R1)
      (value 470)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC850))
    (comp (ref C12)
      (value 330pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71H331KA01D)
        (field (name Description) "CAP CER 330PF 50V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC84D))
    (comp (ref C42)
      (value 100pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAEC781))
    (comp (ref C26)
      (value 47pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JA01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAA149B))
    (comp (ref C30)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4FAA0C67))
    (comp (ref U3)
      (value RX_LOWPASS_FILTER)
      (footprint hackrf:GSG-LP0603)
      (fields
        (field (name Manufacturer) AVX)
        (field (name "Part Number") LP0603A1880ANTR)
        (field (name Description) "FILTER LOW PASS 1880MHZ 0603 SMD"))
      (libsource (lib hackrf) (part FIL-LP0603))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4F94D561))
    (comp (ref U8)
      (value RX_HIGHPASS_FILTER)
      (footprint hackrf:GSG-HP-DEA)
      (fields
        (field (name Manufacturer) TDK)
        (field (name "Part Number") DEA162400HT-8004B1)
        (field (name Description) "FILTER HIGHPASS WLAN&BLUETOOTH"))
      (libsource (lib hackrf) (part FIL-DEA))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4F94D4F4))
    (comp (ref P4)
      (value ANTENNA)
      (footprint hackrf:GSG-SMA-73251-2120)
      (fields
        (field (name Manufacturer) Molex)
        (field (name "Part Number") 73251-2121)
        (field (name Description) "CONN SMA JACK 50 OHM EDGE MNT W/JAM NUT & LOCK WASHER"))
      (libsource (lib hackrf) (part GSG-RF-CONN))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 4F94D0F2))
    (comp (ref P6)
      (value GPO4)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 526B7056))
    (comp (ref J2)
      (value RF-SHIELD-FRAME)
      (footprint hackrf:GSG-SHIELD-BMI-S-230)
      (fields
        (field (name Manufacturer) Laird)
        (field (name "Part Number") BMI-S-230-F-R)
        (field (name Description) "BOARD SHIELD 2INX1.5IN FRAME")
        (field (name Note) DNP))
      (libsource (lib hackrf) (part RF-SHIELD-FRAME))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 527E97CF))
    (comp (ref J3)
      (value RF-SHIELD-COVER)
      (footprint hackrf:GSG-NULL-MODULE)
      (fields
        (field (name Manufacturer) Laird)
        (field (name "Part Number") BMI-S-230-C)
        (field (name Description) "BOARD SHIELD 2INX1.5IN COVER")
        (field (name Note) DNP))
      (libsource (lib hackrf) (part RF-SHIELD-COVER))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 527EAA54))
    (comp (ref P19)
      (value GPO3)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 5280432B))
    (comp (ref P7)
      (value GPO2)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528044D2))
    (comp (ref P13)
      (value GPO1)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528044D9))
    (comp (ref P21)
      (value REF_IN)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528044E0))
    (comp (ref P17)
      (value GPO6)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805038))
    (comp (ref P27)
      (value MIXER_SDATA)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528054F2))
    (comp (ref P31)
      (value MIXER_SCLK)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528054F9))
    (comp (ref P32)
      (value MIXER_ENX)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805500))
    (comp (ref P33)
      (value MIXER_RESETX)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805507))
    (comp (ref P34)
      (value MIX_BYPASS)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C27))
    (comp (ref P35)
      (value !MIX_BYPASS)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C2E))
    (comp (ref P42)
      (value TX)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C35))
    (comp (ref P43)
      (value RX)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C3C))
    (comp (ref P44)
      (value HP)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C47))
    (comp (ref P45)
      (value LP)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C4E))
    (comp (ref P46)
      (value TX_MIX_BP)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C55))
    (comp (ref P47)
      (value RX_MIX_BP)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C5C))
    (comp (ref P48)
      (value TX_AMP)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C67))
    (comp (ref P49)
      (value RX_AMP)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C6E))
    (comp (ref P50)
      (value AMP_BYPASS)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C75))
    (comp (ref P51)
      (value !TX_AMP_PWR)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C7C))
    (comp (ref P52)
      (value !RX_AMP_PWR)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52805C87))
    (comp (ref C166)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 5281BF94))
    (comp (ref C58)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528EA8DE))
    (comp (ref C50)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528EA90E))
    (comp (ref C59)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528EA93E))
    (comp (ref C62)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528EA96E))
    (comp (ref J4)
      (value MOUNTING_HOLE)
      (footprint hackrf:GSG-HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528FA040))
    (comp (ref J5)
      (value MOUNTING_HOLE)
      (footprint hackrf:GSG-HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528FA22A))
    (comp (ref J6)
      (value MOUNTING_HOLE)
      (footprint hackrf:GSG-HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528FA29A))
    (comp (ref J7)
      (value MOUNTING_HOLE)
      (footprint hackrf:GSG-HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528FA2A8))
    (comp (ref J8)
      (value MOUNTING_HOLE)
      (footprint hackrf:GSG-HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528FA2B6))
    (comp (ref J9)
      (value MOUNTING_HOLE)
      (footprint hackrf:GSG-HOLE126MIL-COPPER)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 528FA2C4))
    (comp (ref C67)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52901196))
    (comp (ref C70)
      (value 100pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 529011D6))
    (comp (ref J10)
      (value GND_CLIP)
      (footprint hackrf:GSG-TEST-POINT-S1751-46R)
      (fields
        (field (name Manufacturer) Harwin)
        (field (name "Part Number") S1751-46R)
        (field (name Description) "PC TEST POINT TIN SMD")
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 5293FD15))
    (comp (ref R36)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52EA1180))
    (comp (ref L13)
      (value 10uH)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T100M)
        (field (name Description) "INDUCTR 10UH 220MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52EA1189))
    (comp (ref C171)
      (value 1uF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ105KV-F)
        (field (name Description) "CAP CER 1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 52EA119B))
    (comp (ref L11)
      (value 10uH)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T100M)
        (field (name Description) "INDUCTR 10UH 220MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 57E4FFD8))
    (comp (ref U20)
      (value AP2553W6-7)
      (footprint gsg-modules:SOT457)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") AP2553W6-7)
        (field (name Description) "IC PD SW CURR LIMIT SOT26"))
      (libsource (lib gsg-symbols) (part NX5P2553GV))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 57E6AE8D))
    (comp (ref R33)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 57E6E64A))
    (comp (ref P3)
      (value ANT_FAULT)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /frontend/) (tstamps /503BB638/))
      (tstamp 57E76694))
    (comp (ref R28)
      (value 1k8)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT1K80)
        (field (name Description) "RES TF 1.8K OHM 5% 1/16W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 50549522))
    (comp (ref R85)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD")
        (field (name Note) DNP))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5052A7D7))
    (comp (ref P40)
      (value SSP0_MOSI)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5052A336))
    (comp (ref P41)
      (value SSP0_MISO)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5052A335))
    (comp (ref P39)
      (value SSP0_SCK)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5052A332))
    (comp (ref P36)
      (value VAA)
      (footprint hackrf:GSG-HEADER-1x2)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_2))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5048D547))
    (comp (ref C90)
      (value 100pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H101JA01D)
        (field (name Description) "CAP CER 100PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F929C))
    (comp (ref C102)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F914F))
    (comp (ref C99)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F9135))
    (comp (ref C94)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8F5D))
    (comp (ref C86)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8F4E))
    (comp (ref C85)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F8F4D))
    (comp (ref C105)
      (value 10uF)
      (footprint hackrf:GSG-0805)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM21BR61A106KE19L)
        (field (name Description) "CAP CER 10UF 10V 10% X5R 0805"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F888A))
    (comp (ref FB2)
      (value FILTER)
      (footprint hackrf:GSG-0805)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") BLM21PG221SN1D)
        (field (name Description) "FERRITE CHIP 220 OHM 2000MA 0805"))
      (libsource (lib device) (part FILTER))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503F885C))
    (comp (ref C112)
      (value 180pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H181JA01D)
        (field (name Description) "CAP CER 180PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C527F))
    (comp (ref C91)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4B4A))
    (comp (ref R104)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4AC5))
    (comp (ref R41)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4ABC))
    (comp (ref R105)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4AB0))
    (comp (ref C93)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4A4B))
    (comp (ref C92)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4A4A))
    (comp (ref C89)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4A48))
    (comp (ref C88)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4A45))
    (comp (ref C87)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C4A38))
    (comp (ref C122)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49CE))
    (comp (ref C121)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49CD))
    (comp (ref C120)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49CC))
    (comp (ref C119)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49AF))
    (comp (ref C113)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 503C49A8))
    (comp (ref P15)
      (value INTR)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5037A16F))
    (comp (ref P18)
      (value OEB)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5037A131))
    (comp (ref P14)
      (value XCVR_CLKOUT)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 50371714))
    (comp (ref U17)
      (value MAX2837)
      (footprint hackrf:GSG-QFN48-6)
      (fields
        (field (name Manufacturer) Maxim)
        (field (name "Part Number") MAX2837ETM+)
        (field (name Description) "IC TXRX 2.3GHZ-2.7GHZ 48TQFN"))
      (libsource (lib hackrf) (part MAX2837))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BBC9D))
    (comp (ref L8)
      (value DNP)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D6AFA))
    (comp (ref L9)
      (value DNP)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D6AD6))
    (comp (ref L6)
      (value DNP)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D6AAA))
    (comp (ref X1)
      (value GSG-XTAL4PIN)
      (footprint hackrf:GSG-XTAL3.2x2.5mm)
      (fields
        (field (name Manufacturer) AVX)
        (field (name "Part Number") CX3225GB25000D0HEQZ1)
        (field (name Description) "CRYSTAL 25.000MHZ 8PF SMD")
        (field (name Note) DNP))
      (libsource (lib hackrf) (part GSG-XTAL4PIN))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D0B05))
    (comp (ref R27)
      (value 1k8)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT1K80)
        (field (name Description) "RES TF 1.8K OHM 5% 1/16W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D0602))
    (comp (ref U19)
      (value SI5351C)
      (footprint hackrf:GSG-QFN20-4)
      (fields
        (field (name Manufacturer) "Silicon Laboratories Inc")
        (field (name "Part Number") SI5351C-B-GM)
        (field (name Description) "IC CLK GENERATOR 160MHZ 20QFN"))
      (libsource (lib hackrf) (part SI5351C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5D0564))
    (comp (ref T4)
      (value TX_BALUN)
      (footprint hackrf:GSG-2500BL14M100)
      (fields
        (field (name Manufacturer) "Johanson Technology")
        (field (name "Part Number") 2500BL14M100T)
        (field (name Description) "BALUN CERAMIC CHIP WIMAX 2.5GHZ"))
      (libsource (lib hackrf) (part BALUN))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BDC0F))
    (comp (ref T3)
      (value RX_BALUN)
      (footprint hackrf:GSG-2500BL14M100)
      (fields
        (field (name Manufacturer) "Johanson Technology")
        (field (name "Part Number") 2500BL14M100T)
        (field (name Description) "BALUN CERAMIC CHIP WIMAX 2.5GHZ"))
      (libsource (lib hackrf) (part BALUN))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BDB90))
    (comp (ref C104)
      (value 3pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H3R0CA01D)
        (field (name Description) "CAP CER 3PF 50V NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BD68E))
    (comp (ref C111)
      (value 3pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H3R0CA01D)
        (field (name Description) "CAP CER 3PF 50V NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BD678))
    (comp (ref C106)
      (value 1uF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ105KV-F)
        (field (name Description) "CAP CER 1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC172))
    (comp (ref R26)
      (value 475)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC065))
    (comp (ref R25)
      (value 475)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC059))
    (comp (ref C114)
      (value 3.3nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71H332KA01D)
        (field (name Description) "CAP CER 3300PF 50V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BC057))
    (comp (ref L7)
      (value 6.2nH)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") HK10056N2S-T)
        (field (name Description) "INDUCTOR HIFREQ 6.2+/-0.3NH 0402"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BBD57))
    (comp (ref C84)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 4F5BBD0A))
    (comp (ref Q3)
      (value MOSFET_P)
      (footprint gsg-modules:SOT23GDS)
      (fields
        (field (name Manufacturer) "Diodes Inc.")
        (field (name "Part Number") DMP2305U-7)
        (field (name Description) "MOSFET P-CH 20V 4.2A SOT-23"))
      (libsource (lib neapolitan-cache) (part MOSFET_P))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 526AF6D0))
    (comp (ref R11)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 526AF8E4))
    (comp (ref P55)
      (value TXENABLE)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52806F80))
    (comp (ref P56)
      (value RXENABLE)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52806F87))
    (comp (ref P53)
      (value CS_XCVR)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52806F99))
    (comp (ref P57)
      (value XTAL2)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52807566))
    (comp (ref P67)
      (value RSSI)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5280A12A))
    (comp (ref C167)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281B72F))
    (comp (ref P83)
      (value GND)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281C7E9))
    (comp (ref P84)
      (value GND)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281C9AD))
    (comp (ref P85)
      (value GND)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281C9BB))
    (comp (ref P86)
      (value GND)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281C9C9))
    (comp (ref P87)
      (value GND)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281C9D7))
    (comp (ref P88)
      (value GND)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281C9E5))
    (comp (ref P89)
      (value GND)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281C9F3))
    (comp (ref P90)
      (value GND)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281CA01))
    (comp (ref P91)
      (value GND)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281CEEC))
    (comp (ref P92)
      (value GND)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5281CEFA))
    (comp (ref C115)
      (value 33pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H330JA01D)
        (field (name Description) "CAP CER 33PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5290226B))
    (comp (ref C116)
      (value 47pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H470JA01D)
        (field (name Description) "CAP CER 47PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52902274))
    (comp (ref P9)
      (value BASEBAND)
      (footprint hackrf:GSG-HEADER-2x8)
      (fields
        (field (name Manufacturer) Sullins)
        (field (name "Part Number") PPPC082LFBN-RC)
        (field (name Description) "CONN HEADER FMAL 16PS.1\" DL GOLD"))
      (libsource (lib neapolitan-cache) (part CONN_8X2))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 5294060F))
    (comp (ref C169)
      (value DNP)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52AA5602))
    (comp (ref C170)
      (value DNP)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 52AA5635))
    (comp (ref L15)
      (value 10uH)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T100M)
        (field (name Description) "INDUCTR 10UH 220MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 57E4138B))
    (comp (ref L16)
      (value 10uH)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T100M)
        (field (name Description) "INDUCTR 10UH 220MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 57E43380))
    (comp (ref L14)
      (value 10uH)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T100M)
        (field (name Description) "INDUCTR 10UH 220MA 20% 0603 SMD"))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 57E47605))
    (comp (ref C80)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 57E63DCE))
    (comp (ref C81)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /baseband/) (tstamps /50370666/))
      (tstamp 57E63EF1))
    (comp (ref R75)
      (value 470)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 503C51A8))
    (comp (ref D5)
      (value RXLED)
      (footprint gsg-modules:LTST-S220)
      (fields
        (field (name Manufacturer) Lite-On)
        (field (name "Part Number") LTST-S220KSKT)
        (field (name Description) "LED YELLOW CLEAR RT ANG 0805"))
      (libsource (lib device) (part LED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F83C276))
    (comp (ref D7)
      (value VCCLED)
      (footprint gsg-modules:LTST-S220)
      (fields
        (field (name Manufacturer) Lite-On)
        (field (name "Part Number") LTST-S220KGKT)
        (field (name Description) "LED GREEN CLEAR RT ANG 0805"))
      (libsource (lib device) (part LED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F83C1D6))
    (comp (ref D6)
      (value TXLED)
      (footprint gsg-modules:LTST-S220)
      (fields
        (field (name Manufacturer) Lite-On)
        (field (name "Part Number") LTST-S220KRKT)
        (field (name Description) "LED SUPR RED CLR RT ANG 0805"))
      (libsource (lib device) (part LED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F83C1A7))
    (comp (ref P28)
      (value SD)
      (footprint hackrf:GSG-HEADER-2x11)
      (fields
        (field (name Manufacturer) Sullins)
        (field (name "Part Number") PPPC112LFBN-RC)
        (field (name Description) "CONN HEADER FMAL 22PS.1\" DL GOLD"))
      (libsource (lib hackrf) (part CONN_11X2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F837D97))
    (comp (ref FB1)
      (value FILTER)
      (footprint hackrf:GSG-0805)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") BLM21PG221SN1D)
        (field (name Description) "FERRITE CHIP 220 OHM 2000MA 0805"))
      (libsource (lib device) (part FILTER))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F766F5E))
    (comp (ref J1)
      (value USB-MICRO-B)
      (footprint hackrf:GSG-USB-MICROB-FCI-10103592-EXT)
      (fields
        (field (name Manufacturer) FCI)
        (field (name "Part Number") 10103592-0001LF)
        (field (name Description) "CONN RCPT REV MICRO USB TYPE B"))
      (libsource (lib hackrf) (part GSG-USB-MICRO-B-SHIELDED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F766BDF))
    (comp (ref P22)
      (value I2S)
      (footprint hackrf:GSG-HEADER-2x13)
      (fields
        (field (name Manufacturer) Sullins)
        (field (name "Part Number") PPPC132LFBN-RC)
        (field (name Description) "CONN HEADER FMAL 26PS.1\" DL GOLD"))
      (libsource (lib neapolitan-cache) (part CONN_13X2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 526B4073))
    (comp (ref D2)
      (value VAALED)
      (footprint gsg-modules:LTST-S220)
      (fields
        (field (name Manufacturer) Lite-On)
        (field (name "Part Number") LTST-S220KRKT)
        (field (name Description) "LED SUPR RED CLR RT ANG 0805"))
      (libsource (lib device) (part LED))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 527DC2E9))
    (comp (ref P5)
      (value LEDS)
      (footprint hackrf:GSG-HEADER-2x3)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_3X2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 528023DB))
    (comp (ref P80)
      (value SHIELD)
      (footprint hackrf:GSG-HEADER-NOMARK-1x2)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 528064FC))
    (comp (ref R35)
      (value DNP)
      (footprint hackrf:GSG-0805)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5294026C))
    (comp (ref C155)
      (value DNP)
      (footprint hackrf:GSG-0805)
      (fields
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5294027B))
    (comp (ref R73)
      (value 1k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402FT1K00)
        (field (name Description) "RES 1K OHM 1/16W 1% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5298FBA8))
    (comp (ref R74)
      (value 1k8)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT1K80)
        (field (name Description) "RES TF 1.8K OHM 5% 1/16W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 5299055B))
    (comp (ref R18)
      (value 1k8)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT1K80)
        (field (name Description) "RES TF 1.8K OHM 5% 1/16W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 529905C9))
    (comp (ref FB3)
      (value FILTER)
      (footprint hackrf:GSG-0805)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") BLM21PG221SN1D)
        (field (name Description) "FERRITE CHIP 220 OHM 2000MA 0805"))
      (libsource (lib device) (part FILTER))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 52EA190B))
    (comp (ref R7)
      (value 470)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT470R)
        (field (name Description) "RES TF 1/16W 470 OHM 5% 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CA8054))
    (comp (ref J11)
      (value BARREL_JACK)
      (footprint gsg-modules:CUI_PJ-102[AB]H)
      (fields
        (field (name Manufacturer) CUI)
        (field (name "Part Number") PJ-102AH)
        (field (name Description) "CONN PWR JACK 2.0X5.5MM HIGH CUR "))
      (libsource (lib conn) (part BARREL_JACK))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CB0AF2))
    (comp (ref D10)
      (value VIN_DIODE)
      (footprint gsg-modules:SOD128)
      (fields
        (field (name Manufacturer) NXP)
        (field (name "Part Number") PMEG3050EP,115)
        (field (name Description) "DIODE SCHOTTKY 30V 5A SOD128"))
      (libsource (lib device) (part D_Schottky))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CB4E5A))
    (comp (ref D4)
      (value BARREL_DIODE)
      (footprint gsg-modules:SOD128)
      (fields
        (field (name Manufacturer) NXP)
        (field (name "Part Number") PMEG3050EP,115)
        (field (name Description) "DIODE SCHOTTKY 30V 5A SOD128"))
      (libsource (lib device) (part D_Schottky))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CB4ECD))
    (comp (ref U15)
      (value TCA6424A)
      (footprint gsg-modules:QFN32-5)
      (fields
        (field (name Manufacturer) "Texas Instruments")
        (field (name "Part Number") TCA6424ARGJR)
        (field (name Description) "I/O Expander 24 I²C, SMBus 400kHz 32-UQFN Exposed Pad (5x5) "))
      (libsource (lib gsg-symbols) (part TCA6424A))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CAD041))
    (comp (ref R8)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CB915E))
    (comp (ref R9)
      (value 18k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Yageo)
        (field (name "Part Number") RC0402JR-0718KL)
        (field (name Description) "RES SMD 18K OHM 5% 1/16W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CB93F4))
    (comp (ref D8)
      (value VBUS2_DIODE)
      (footprint gsg-modules:SOD128)
      (fields
        (field (name Manufacturer) NXP)
        (field (name "Part Number") PMEG3050EP,115)
        (field (name Description) "DIODE SCHOTTKY 30V 5A SOD128"))
      (libsource (lib device) (part D_Schottky))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CA7813))
    (comp (ref R13)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CBA6DD))
    (comp (ref R14)
      (value 18k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Yageo)
        (field (name "Part Number") RC0402JR-0718KL)
        (field (name Description) "RES SMD 18K OHM 5% 1/16W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CBA6E6))
    (comp (ref R10)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CBB468))
    (comp (ref R12)
      (value 18k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Yageo)
        (field (name "Part Number") RC0402JR-0718KL)
        (field (name Description) "RES SMD 18K OHM 5% 1/16W 0402"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CBB471))
    (comp (ref R16)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CBDD42))
    (comp (ref P2)
      (value !IO_RESET)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CBE373))
    (comp (ref R15)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CBEA99))
    (comp (ref P1)
      (value !IO_INT)
      (footprint hackrf:GSG-TESTPOINT-50MIL)
      (fields
        (field (name Note) DNP))
      (libsource (lib neapolitan-cache) (part CONN_1))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CBEAA0))
    (comp (ref X2)
      (value FOX924B)
      (footprint gsg-modules:XTAL5.0x3.2mm)
      (fields
        (field (name Manufacturer) "Fox Electronics")
        (field (name "Part Number") FOX924B-10.000)
        (field (name Description) "OSC TCXO 10.000MHZ HCMOS SMD"))
      (libsource (lib gsg-symbols) (part FOX924B))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CDD95C))
    (comp (ref R17)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CE0CD6))
    (comp (ref Q5)
      (value MOSFET_P)
      (footprint gsg-modules:SOT23GDS)
      (fields
        (field (name Manufacturer) Fairchild)
        (field (name "Part Number") BSS84)
        (field (name Description) "MOSFET P-CH 50V 130MA SOT-23"))
      (libsource (lib neapolitan-cache) (part MOSFET_P))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CE0CF4))
    (comp (ref C68)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CE1C4F))
    (comp (ref R19)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD")
        (field (name Note) DNP))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CE5098))
    (comp (ref R20)
      (value 0)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402ZT0R00)
        (field (name Description) "RES 0.0 OHM 1/16W 0402 SMD")
        (field (name Note) DNP))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CE5E04))
    (comp (ref X3)
      (value KT2520)
      (footprint gsg-modules:KT2520K)
      (fields
        (field (name Manufacturer) AVX)
        (field (name "Part Number") KT2520K26000ACW18TAS)
        (field (name Description) "TCXO Oscillators 26MHz 1.8Volts 2.5mmx2mm"))
      (libsource (lib gsg-symbols) (part KT2520))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CE8B5F))
    (comp (ref C71)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CEA3A2))
    (comp (ref C69)
      (value 1uF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") LMK105BJ105KV-F)
        (field (name Description) "CAP CER 1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CEB526))
    (comp (ref U16)
      (value TCR2EF)
      (footprint gsg-modules:SOT25)
      (fields
        (field (name Manufacturer) Toshiba)
        (field (name "Part Number") "TCR2EF33,LM(CT")
        (field (name Description) "IC REG LDO 3.3V 0.2A SMV"))
      (libsource (lib gsg-symbols) (part TCR2EF))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CEC4F7))
    (comp (ref C72)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57CED4AD))
    (comp (ref U18)
      (value 74LVC1G14)
      (footprint gsg-modules:SOT353-1)
      (fields
        (field (name Manufacturer) NXP)
        (field (name "Part Number") 74LVC1G14GW,125)
        (field (name Description) "Inverter IC 1 Channel Schmitt Trigger 5-TSSOP"))
      (libsource (lib 74xx) (part 74AHC1G14))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E2187A))
    (comp (ref Q6)
      (value MOSFET_P)
      (footprint gsg-modules:SOT23GDS)
      (fields
        (field (name Manufacturer) Fairchild)
        (field (name "Part Number") BSS84)
        (field (name Description) "MOSFET P-CH 50V 130MA SOT-23"))
      (libsource (lib neapolitan-cache) (part MOSFET_P))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E22D08))
    (comp (ref R30)
      (value 470k)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) Yageo)
        (field (name "Part Number") RC0603JR-07470KL)
        (field (name Description) "RES SMD 470K OHM 5% 1/10W 0603"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E266DB))
    (comp (ref C74)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E26F7F))
    (comp (ref R31)
      (value 470k)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) Yageo)
        (field (name "Part Number") RC0603JR-07470KL)
        (field (name Description) "RES SMD 470K OHM 5% 1/10W 0603"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E27358))
    (comp (ref C73)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402")
        (field (name Note) DNP))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E2A0BE))
    (comp (ref R23)
      (value 470k)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) Yageo)
        (field (name "Part Number") RC0603JR-07470KL)
        (field (name Description) "RES SMD 470K OHM 5% 1/10W 0603")
        (field (name Note) DNP))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E2A0CE))
    (comp (ref L10)
      (value 10uH)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) "Taiyo Yuden")
        (field (name "Part Number") BRL1608T100M)
        (field (name Description) "INDUCTR 10UH 220MA 20% 0603 SMD")
        (field (name Note) DNP))
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E2AEC1))
    (comp (ref R22)
      (value 470k)
      (footprint hackrf:GSG-0603)
      (fields
        (field (name Manufacturer) Yageo)
        (field (name "Part Number") RC0603JR-07470KL)
        (field (name Description) "RES SMD 470K OHM 5% 1/10W 0603")
        (field (name Note) DNP))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E2C011))
    (comp (ref R21)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E30224))
    (comp (ref X4)
      (value OH4)
      (footprint gsg-modules:OH4)
      (fields
        (field (name Manufacturer) Connor-Winfield)
        (field (name "Part Number") OH4610LF-010.0M)
        (field (name Description) "10MHz LVCMOS OCXO Oscillator Through Hole 3.3V"))
      (libsource (lib gsg-symbols) (part OH4))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E3681D))
    (comp (ref Q7)
      (value MOSFET_P)
      (footprint gsg-modules:SOT23GDS)
      (fields
        (field (name Manufacturer) Fairchild)
        (field (name "Part Number") BSS84)
        (field (name Description) "MOSFET P-CH 50V 130MA SOT-23"))
      (libsource (lib neapolitan-cache) (part MOSFET_P))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E36AF3))
    (comp (ref R32)
      (value 10k)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Stackpole)
        (field (name "Part Number") RMCF0402JT10K0)
        (field (name Description) "RES 10K OHM 1/16W 5% 0402 SMD"))
      (libsource (lib device) (part R))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E36AFC))
    (comp (ref C76)
      (value 10nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R71C103KA01D)
        (field (name Description) "CAP CER 10000PF 16V 10% X7R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E3966F))
    (comp (ref C75)
      (value 22pF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM1555C1H220JA01D)
        (field (name Description) "CAP CER 22PF 50V 5% NP0 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E3C654))
    (comp (ref P20)
      (value GPIO)
      (footprint hackrf:GSG-HEADER-2x11)
      (fields
        (field (name Manufacturer) Sullins)
        (field (name "Part Number") PPPC112LFBN-RC)
        (field (name Description) "CONN HEADER FMAL 22PS.1\" DL GOLD"))
      (libsource (lib hackrf) (part CONN_11X2))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 4F838167))
    (comp (ref C79)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E5BCE3))
    (comp (ref C78)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E5DB21))
    (comp (ref C77)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E5DEBE))
    (comp (ref C82)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E5FDFF))
    (comp (ref C83)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E60E4F))
    (comp (ref C95)
      (value 100nF)
      (footprint hackrf:GSG-0402)
      (fields
        (field (name Manufacturer) Murata)
        (field (name "Part Number") GRM155R61A104KA01D)
        (field (name Description) "CAP CER 0.1UF 10V 10% X5R 0402"))
      (libsource (lib device) (part C))
      (sheetpath (names /mcu/usb/power/) (tstamps /5037043E/))
      (tstamp 57E620CE)))
  (libparts
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part INDUCTOR)
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-3MM)
        (fp LED-5MM)
        (fp LED-10MM)
        (fp LED-0603)
        (fp LED-0805)
        (fp LED-1206)
        (fp LEDV))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib hackrf) (part MGA-81563)
      (fields
        (field (name Reference) U)
        (field (name Value) MGA-81563))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name IN) (type input))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name OUT) (type output))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib hackrf) (part GSG-USB-MICRO-B-SHIELDED)
      (fields
        (field (name Reference) J)
        (field (name Value) GSG-USB-MICRO-B-SHIELDED))
      (pins
        (pin (num 0) (name SHIELD) (type passive))
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type BiDi))
        (pin (num 3) (name D+) (type BiDi))
        (pin (num 4) (name ID) (type input))
        (pin (num 5) (name GND) (type power_out))))
    (libpart (lib hackrf) (part RF-SHIELD-COVER)
      (fields
        (field (name Reference) J)
        (field (name Value) RF-SHIELD-COVER)))
    (libpart (lib gsg-symbols) (part TCR2EF)
      (fields
        (field (name Reference) U)
        (field (name Value) TCR2EF))
      (pins
        (pin (num 1) (name VIN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name CTRL) (type input))
        (pin (num 4) (name NC) (type NotConnected))
        (pin (num 5) (name VOUT) (type power_out))))
    (libpart (lib hackrf) (part SKY13317)
      (fields
        (field (name Reference) U)
        (field (name Value) SKY13317))
      (pins
        (pin (num 0) (name GND) (type power_in))
        (pin (num 1) (name RFC) (type BiDi))
        (pin (num 2) (name NC) (type NotConnected))
        (pin (num 3) (name V1) (type input))
        (pin (num 4) (name RF1) (type BiDi))
        (pin (num 5) (name RF2) (type BiDi))
        (pin (num 6) (name V2) (type input))
        (pin (num 7) (name V3) (type input))
        (pin (num 8) (name RF3) (type BiDi))))
    (libpart (lib device) (part D_Schottky)
      (description "Diode schottky")
      (footprints
        (fp D-Pak_TO252AA)
        (fp Diode_*)
        (fp *SingleDiode)
        (fp *SingleDiode*)
        (fp *_Diode_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib conn) (part BARREL_JACK)
      (description "DC Barrel Jack")
      (fields
        (field (name Reference) CON)
        (field (name Value) BARREL_JACK))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))))
    (libpart (lib device) (part FILTER)
      (description "Filtre EMI")
      (fields
        (field (name Reference) FB)
        (field (name Value) FILTER))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib hackrf) (part CONN_11X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_11X2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))))
    (libpart (lib neapolitan-cache) (part CONN_13X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_13X2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))
        (pin (num 13) (name P13) (type passive))
        (pin (num 14) (name P14) (type passive))
        (pin (num 15) (name P15) (type passive))
        (pin (num 16) (name P16) (type passive))
        (pin (num 17) (name P17) (type passive))
        (pin (num 18) (name P18) (type passive))
        (pin (num 19) (name P19) (type passive))
        (pin (num 20) (name P20) (type passive))
        (pin (num 21) (name P21) (type passive))
        (pin (num 22) (name P22) (type passive))
        (pin (num 23) (name P23) (type passive))
        (pin (num 24) (name P20) (type passive))
        (pin (num 25) (name P24) (type passive))
        (pin (num 26) (name P22) (type passive))))
    (libpart (lib hackrf) (part MAX2837)
      (fields
        (field (name Reference) U)
        (field (name Value) MAX2837))
      (pins
        (pin (num 0) (name EP) (type power_in))
        (pin (num 1) (name VCCRXLNA) (type power_in))
        (pin (num 2) (name GNDRXLNA) (type power_in))
        (pin (num 3) (name B5) (type input))
        (pin (num 4) (name RXRF+) (type input))
        (pin (num 5) (name RXRF-) (type input))
        (pin (num 6) (name B4) (type input))
        (pin (num 7) (name VCCTXPAD) (type power_in))
        (pin (num 8) (name B3) (type input))
        (pin (num 9) (name B2) (type input))
        (pin (num 10) (name TXRF+) (type output))
        (pin (num 11) (name TXRF-) (type output))
        (pin (num 12) (name B1) (type input))
        (pin (num 13) (name VCCTXMX) (type power_in))
        (pin (num 14) (name PABIAS) (type output))
        (pin (num 15) (name SCLK) (type input))
        (pin (num 16) (name CLOCKOUT) (type output))
        (pin (num 17) (name XTAL2) (type input))
        (pin (num 18) (name XTAL1) (type output))
        (pin (num 19) (name VCCXTAL) (type power_in))
        (pin (num 20) (name VCCDIG) (type power_in))
        (pin (num 21) (name VCCCP) (type power_in))
        (pin (num 22) (name GNDCP) (type power_in))
        (pin (num 23) (name CPOUT+) (type output))
        (pin (num 24) (name CPOUT-) (type output))
        (pin (num 25) (name ENABLE) (type input))
        (pin (num 26) (name GNDVCO) (type power_in))
        (pin (num 27) (name BYPASS) (type output))
        (pin (num 28) (name VCCVCO) (type power_in))
        (pin (num 29) (name DOUT) (type output))
        (pin (num 30) (name CS) (type input))
        (pin (num 31) (name DIN) (type input))
        (pin (num 32) (name RSSI) (type output))
        (pin (num 33) (name B7) (type input))
        (pin (num 34) (name B6) (type input))
        (pin (num 35) (name RXBBQ-) (type output))
        (pin (num 36) (name RXBBQ+) (type output))
        (pin (num 37) (name RXBBI-) (type output))
        (pin (num 38) (name RXBBI+) (type output))
        (pin (num 39) (name VCCRXVGA) (type power_in))
        (pin (num 40) (name RXHP) (type input))
        (pin (num 41) (name VCCRXFL) (type power_in))
        (pin (num 42) (name TXBBI-) (type input))
        (pin (num 43) (name TXBBI+) (type input))
        (pin (num 44) (name TXBBQ+) (type input))
        (pin (num 45) (name TXBBQ-) (type input))
        (pin (num 46) (name VCCRXMX) (type power_in))
        (pin (num 47) (name TXENABLE) (type input))
        (pin (num 48) (name RXENABLE) (type input))))
    (libpart (lib gsg-symbols) (part FOX924B)
      (fields
        (field (name Reference) X)
        (field (name Value) FOX924B))
      (pins
        (pin (num 1) (name NC) (type NotConnected))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type output))
        (pin (num 4) (name VCC) (type power_in))))
    (libpart (lib gsg-symbols) (part OH4)
      (fields
        (field (name Reference) X)
        (field (name Value) OH4))
      (pins
        (pin (num 1) (name NC/VC) (type input))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name OUT) (type output))
        (pin (num 14) (name VCC) (type power_in))))
    (libpart (lib gsg-symbols) (part KT2520)
      (fields
        (field (name Reference) X)
        (field (name Value) KT2520))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name NC) (type NotConnected))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name OUT) (type output))
        (pin (num 5) (name NC) (type NotConnected))
        (pin (num 6) (name VCC) (type power_in))))
    (libpart (lib neapolitan-cache) (part CONN_8X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_8X2))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name ~) (type passive))
        (pin (num 10) (name ~) (type passive))
        (pin (num 11) (name ~) (type passive))
        (pin (num 12) (name ~) (type passive))
        (pin (num 13) (name ~) (type passive))
        (pin (num 14) (name ~) (type passive))
        (pin (num 15) (name ~) (type passive))
        (pin (num 16) (name ~) (type passive))))
    (libpart (lib hackrf) (part SI5351C)
      (fields
        (field (name Reference) U)
        (field (name Value) SI5351C))
      (pins
        (pin (num 0) (name GND) (type power_in))
        (pin (num 1) (name XA) (type input))
        (pin (num 2) (name XB) (type input))
        (pin (num 3) (name INTR) (type output))
        (pin (num 4) (name SCL) (type input))
        (pin (num 5) (name SDA) (type BiDi))
        (pin (num 6) (name CLKIN) (type input))
        (pin (num 7) (name OEB) (type input))
        (pin (num 8) (name CLK3) (type output))
        (pin (num 9) (name CLK2) (type output))
        (pin (num 10) (name VDDOB) (type power_in))
        (pin (num 11) (name VDDOA) (type power_in))
        (pin (num 12) (name CLK1) (type output))
        (pin (num 13) (name CLK0) (type output))
        (pin (num 14) (name VDDOD) (type power_in))
        (pin (num 15) (name CLK7) (type output))
        (pin (num 16) (name CLK6) (type output))
        (pin (num 17) (name CLK5) (type output))
        (pin (num 18) (name VDDOC) (type power_in))
        (pin (num 19) (name CLK4) (type output))
        (pin (num 20) (name VDD) (type power_in))))
    (libpart (lib hackrf) (part BALUN)
      (fields
        (field (name Reference) T)
        (field (name Value) BALUN))
      (pins
        (pin (num 1) (name S1) (type passive))
        (pin (num 2) (name S2) (type passive))
        (pin (num 3) (name PR1) (type passive))
        (pin (num 4) (name PR2) (type passive))
        (pin (num 5) (name PM) (type passive))))
    (libpart (lib gsg-symbols) (part TCA6424A)
      (fields
        (field (name Reference) U)
        (field (name Value) TCA6424A))
      (pins
        (pin (num 0) (name GND) (type power_in))
        (pin (num 1) (name P00) (type BiDi))
        (pin (num 2) (name P01) (type BiDi))
        (pin (num 3) (name P02) (type BiDi))
        (pin (num 4) (name P03) (type BiDi))
        (pin (num 5) (name P04) (type BiDi))
        (pin (num 6) (name P05) (type BiDi))
        (pin (num 7) (name P06) (type BiDi))
        (pin (num 8) (name P07) (type BiDi))
        (pin (num 9) (name P10) (type BiDi))
        (pin (num 10) (name P11) (type BiDi))
        (pin (num 11) (name P12) (type BiDi))
        (pin (num 12) (name P13) (type BiDi))
        (pin (num 13) (name P14) (type BiDi))
        (pin (num 14) (name P15) (type BiDi))
        (pin (num 15) (name P16) (type BiDi))
        (pin (num 16) (name P17) (type BiDi))
        (pin (num 17) (name P20) (type BiDi))
        (pin (num 18) (name P21) (type BiDi))
        (pin (num 19) (name P22) (type BiDi))
        (pin (num 20) (name P23) (type BiDi))
        (pin (num 21) (name P24) (type BiDi))
        (pin (num 22) (name P25) (type BiDi))
        (pin (num 23) (name P26) (type BiDi))
        (pin (num 24) (name P27) (type BiDi))
        (pin (num 25) (name GND) (type power_in))
        (pin (num 26) (name ADDR) (type input))
        (pin (num 27) (name VCCP) (type power_in))
        (pin (num 28) (name !RESET) (type input))
        (pin (num 29) (name SCL) (type BiDi))
        (pin (num 30) (name SDA) (type BiDi))
        (pin (num 31) (name VCCI) (type power_in))
        (pin (num 32) (name !INT) (type output))))
    (libpart (lib neapolitan-cache) (part CONN_2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib hackrf) (part FIL-DEA)
      (fields
        (field (name Reference) U)
        (field (name Value) FIL-DEA))
      (pins
        (pin (num 1) (name IN) (type BiDi))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name OUT) (type BiDi))
        (pin (num 4) (name GND) (type power_in))))
    (libpart (lib hackrf) (part SKY13350)
      (fields
        (field (name Reference) U)
        (field (name Value) SKY13350))
      (pins
        (pin (num 1) (name VCTL1) (type input))
        (pin (num 2) (name OUT1) (type BiDi))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name OUT2) (type BiDi))
        (pin (num 5) (name VCTL2) (type input))
        (pin (num 6) (name INPUT) (type BiDi))))
    (libpart (lib hackrf) (part RFFC5072)
      (fields
        (field (name Reference) U)
        (field (name Value) RFFC5072))
      (pins
        (pin (num 0) (name EP) (type power_in))
        (pin (num 1) (name ENBL/GPO5) (type BiDi))
        (pin (num 2) (name EXT_LO) (type input))
        (pin (num 3) (name EXT_LO_DEC) (type passive))
        (pin (num 4) (name REXT) (type passive))
        (pin (num 5) (name ANA_VDD1) (type power_in))
        (pin (num 6) (name LFILT1) (type output))
        (pin (num 7) (name LFITLT2) (type output))
        (pin (num 8) (name LFILT3) (type input))
        (pin (num 9) (name MODE/GPO6) (type BiDi))
        (pin (num 10) (name REF_IN) (type input))
        (pin (num 11) (name NC) (type NotConnected))
        (pin (num 12) (name TM) (type power_in))
        (pin (num 13) (name NC) (type NotConnected))
        (pin (num 14) (name NC) (type NotConnected))
        (pin (num 15) (name GPO1/ADD1) (type BiDi))
        (pin (num 16) (name GPO2/ADD2) (type BiDi))
        (pin (num 17) (name NC) (type NotConnected))
        (pin (num 18) (name NC) (type NotConnected))
        (pin (num 19) (name DIG_VDD) (type power_in))
        (pin (num 20) (name NC) (type NotConnected))
        (pin (num 21) (name NC) (type NotConnected))
        (pin (num 22) (name ANA_VDD2) (type power_in))
        (pin (num 23) (name MIX_IPP) (type input))
        (pin (num 24) (name MIX_IPN) (type input))
        (pin (num 25) (name GPO3/FM) (type BiDi))
        (pin (num 26) (name GPO4/LD/DO) (type BiDi))
        (pin (num 27) (name MIX_OPN) (type output))
        (pin (num 28) (name MIX_OPP) (type output))
        (pin (num 29) (name RESETX) (type input))
        (pin (num 30) (name ENX) (type input))
        (pin (num 31) (name SCLK) (type input))
        (pin (num 32) (name SDATA) (type input))))
    (libpart (lib hackrf) (part GSG-RF-CONN)
      (fields
        (field (name Reference) P)
        (field (name Value) GSG-RF-CONN))
      (pins
        (pin (num 1) (name RF) (type BiDi))
        (pin (num 2) (name GND) (type power_in))))
    (libpart (lib hackrf) (part GSG-XTAL4PIN)
      (fields
        (field (name Reference) X)
        (field (name Value) GSG-XTAL4PIN))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib hackrf) (part GSG-DIODE-TVS-BI)
      (description "Diode zener")
      (footprints
        (fp D?)
        (fp SO*)
        (fp SM*))
      (fields
        (field (name Reference) D)
        (field (name Value) GSG-DIODE-TVS-BI))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name K) (type passive))))
    (libpart (lib 74xx) (part 74AHC1G14)
      (description "inverting buffer with Schmitt trigger.")
      (docs 74xx/74ahc_ahct1g14.pdf)
      (fields
        (field (name Reference) U)
        (field (name Value) 74AHC1G14))
      (pins
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name ~) (type output))
        (pin (num 5) (name VCC) (type power_in))))
    (libpart (lib hackrf) (part FIL-LP0603)
      (fields
        (field (name Reference) U)
        (field (name Value) FIL-LP0603))
      (pins
        (pin (num 1) (name OUT) (type BiDi))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name IN) (type BiDi))))
    (libpart (lib neapolitan-cache) (part CONN_3X2)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_3X2))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))
        (pin (num 5) (name 5) (type passive))
        (pin (num 6) (name 6) (type passive))))
    (libpart (lib gsg-symbols) (part NX5P2553GV)
      (fields
        (field (name Reference) U)
        (field (name Value) NX5P2553GV))
      (pins
        (pin (num 1) (name VIN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name FAULT) (type output))
        (pin (num 5) (name ILIM) (type input))
        (pin (num 6) (name VOUT) (type power_out))))
    (libpart (lib neapolitan-cache) (part MOS_P)
      (aliases
        (alias MOSFET_P))
      (fields
        (field (name Reference) Q)
        (field (name Value) MOS_P))
      (pins
        (pin (num D) (name D) (type passive))
        (pin (num G) (name G) (type input))
        (pin (num S) (name S) (type passive))))
    (libpart (lib hackrf) (part BALUN-B0310J50100AHF)
      (fields
        (field (name Reference) T)
        (field (name Value) BALUN-B0310J50100AHF))
      (pins
        (pin (num 1) (name S1) (type passive))
        (pin (num 2) (name S2) (type passive))
        (pin (num 3) (name PR1) (type passive))
        (pin (num 4) (name PR2) (type passive))))
    (libpart (lib neapolitan-cache) (part CONN_1)
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib hackrf) (part RF-SHIELD-FRAME)
      (fields
        (field (name Reference) J)
        (field (name Value) RF-SHIELD-FRAME))
      (pins
        (pin (num 0) (name SHIELD) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/local/share/kicad/library/device.lib))
    (library (logical hackrf)
      (uri /home/mossmann/src/hackrf/hardware/kicad/hackrf.lib))
    (library (logical gsg-symbols)
      (uri /home/mossmann/src/hackrf/hardware/gsg-kicad-lib/gsg-symbols.lib))
    (library (logical neapolitan-cache)
      (uri /home/mossmann/src/hackrf/hardware/neapolitan/neapolitan-cache.lib))
    (library (logical conn)
      (uri /usr/local/share/kicad/library/conn.lib))
    (library (logical 74xx)
      (uri /usr/local/share/kicad/library/74xx.lib)))
  (nets
    (net (code 1) (name "Net-(P22-Pad24)")
      (node (ref P22) (pin 24)))
    (net (code 2) (name "Net-(P22-Pad26)")
      (node (ref P22) (pin 26)))
    (net (code 3) (name I2C1_SCL)
      (node (ref P22) (pin 5))
      (node (ref U15) (pin 29))
      (node (ref U19) (pin 4))
      (node (ref R28) (pin 2)))
    (net (code 4) (name VCC)
      (node (ref U19) (pin 20))
      (node (ref C78) (pin 1))
      (node (ref R104) (pin 1))
      (node (ref R16) (pin 1))
      (node (ref R105) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref R75) (pin 2))
      (node (ref C77) (pin 1))
      (node (ref R27) (pin 1))
      (node (ref Q6) (pin S))
      (node (ref U19) (pin 10))
      (node (ref R32) (pin 2))
      (node (ref P28) (pin 1))
      (node (ref Q7) (pin S))
      (node (ref L11) (pin 2))
      (node (ref C83) (pin 1))
      (node (ref C82) (pin 1))
      (node (ref U19) (pin 11))
      (node (ref U19) (pin 14))
      (node (ref R22) (pin 1))
      (node (ref P22) (pin 11))
      (node (ref C95) (pin 1))
      (node (ref R21) (pin 2))
      (node (ref Q5) (pin S))
      (node (ref R17) (pin 2))
      (node (ref Q3) (pin S))
      (node (ref R6) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref C167) (pin 1))
      (node (ref C122) (pin 1))
      (node (ref C120) (pin 1))
      (node (ref P20) (pin 3))
      (node (ref P5) (pin 2))
      (node (ref U15) (pin 27))
      (node (ref C72) (pin 1))
      (node (ref U16) (pin 1))
      (node (ref R28) (pin 1))
      (node (ref C119) (pin 1))
      (node (ref L15) (pin 2))
      (node (ref U15) (pin 31))
      (node (ref C113) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref L14) (pin 2)))
    (net (code 5) (name /mcu/usb/power/VBUS2)
      (node (ref D8) (pin 2))
      (node (ref FB1) (pin 2))
      (node (ref R13) (pin 1)))
    (net (code 6) (name "Net-(P28-Pad22)")
      (node (ref P28) (pin 22)))
    (net (code 7) (name "Net-(P28-Pad20)")
      (node (ref P28) (pin 20)))
    (net (code 8) (name "Net-(P28-Pad18)")
      (node (ref P28) (pin 18)))
    (net (code 9) (name "Net-(P28-Pad16)")
      (node (ref P28) (pin 16)))
    (net (code 10) (name "Net-(P28-Pad21)")
      (node (ref P28) (pin 21)))
    (net (code 11) (name "Net-(P28-Pad19)")
      (node (ref P28) (pin 19)))
    (net (code 12) (name "Net-(P28-Pad17)")
      (node (ref P28) (pin 17)))
    (net (code 13) (name "Net-(P28-Pad15)")
      (node (ref P28) (pin 15)))
    (net (code 14) (name "Net-(P5-Pad3)")
      (node (ref P5) (pin 3)))
    (net (code 15) (name GND)
      (node (ref C81) (pin 2))
      (node (ref C53) (pin 2))
      (node (ref U17) (pin 2))
      (node (ref U17) (pin 0))
      (node (ref C88) (pin 2))
      (node (ref U17) (pin 22))
      (node (ref C119) (pin 2))
      (node (ref C113) (pin 2))
      (node (ref C120) (pin 2))
      (node (ref C121) (pin 1))
      (node (ref C122) (pin 2))
      (node (ref C87) (pin 2))
      (node (ref U25) (pin 1))
      (node (ref C94) (pin 2))
      (node (ref C85) (pin 2))
      (node (ref C86) (pin 2))
      (node (ref C105) (pin 2))
      (node (ref C90) (pin 2))
      (node (ref C89) (pin 2))
      (node (ref C92) (pin 2))
      (node (ref C93) (pin 2))
      (node (ref R41) (pin 1))
      (node (ref C91) (pin 2))
      (node (ref R85) (pin 2))
      (node (ref P9) (pin 3))
      (node (ref P9) (pin 16))
      (node (ref P9) (pin 14))
      (node (ref P9) (pin 9))
      (node (ref P9) (pin 8))
      (node (ref C169) (pin 1))
      (node (ref P9) (pin 2))
      (node (ref P9) (pin 1))
      (node (ref C116) (pin 2))
      (node (ref P9) (pin 15))
      (node (ref C80) (pin 2))
      (node (ref U17) (pin 26))
      (node (ref U19) (pin 0))
      (node (ref X1) (pin 4))
      (node (ref X1) (pin 2))
      (node (ref P91) (pin 1))
      (node (ref P90) (pin 1))
      (node (ref P89) (pin 1))
      (node (ref P84) (pin 1))
      (node (ref P85) (pin 1))
      (node (ref P83) (pin 1))
      (node (ref C170) (pin 1))
      (node (ref C167) (pin 2))
      (node (ref P92) (pin 1))
      (node (ref T4) (pin 2))
      (node (ref C84) (pin 2))
      (node (ref T4) (pin 5))
      (node (ref C106) (pin 2))
      (node (ref T3) (pin 2))
      (node (ref T3) (pin 5))
      (node (ref J8) (pin 1))
      (node (ref J9) (pin 1))
      (node (ref J10) (pin 1))
      (node (ref C70) (pin 2))
      (node (ref C166) (pin 2))
      (node (ref C33) (pin 2))
      (node (ref C56) (pin 2))
      (node (ref U2) (pin 3))
      (node (ref C22) (pin 1))
      (node (ref U10) (pin 3))
      (node (ref U7) (pin 3))
      (node (ref J6) (pin 1))
      (node (ref J7) (pin 1))
      (node (ref U20) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref P4) (pin 2))
      (node (ref U8) (pin 4))
      (node (ref U8) (pin 2))
      (node (ref J5) (pin 1))
      (node (ref J4) (pin 1))
      (node (ref U20) (pin 5))
      (node (ref R36) (pin 2))
      (node (ref C171) (pin 2))
      (node (ref C42) (pin 2))
      (node (ref U11) (pin 3))
      (node (ref C3) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref U6) (pin 3))
      (node (ref C41) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref U5) (pin 3))
      (node (ref U1) (pin 3))
      (node (ref C16) (pin 2))
      (node (ref U12) (pin 0))
      (node (ref U4) (pin 0))
      (node (ref U4) (pin 12))
      (node (ref C7) (pin 1))
      (node (ref C47) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C37) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref R4) (pin 1))
      (node (ref U9) (pin 0))
      (node (ref U13) (pin 1))
      (node (ref U13) (pin 2))
      (node (ref U13) (pin 4))
      (node (ref U13) (pin 5))
      (node (ref C39) (pin 1))
      (node (ref C52) (pin 2))
      (node (ref U14) (pin 0))
      (node (ref C29) (pin 2))
      (node (ref C66) (pin 1))
      (node (ref C38) (pin 1))
      (node (ref U25) (pin 4))
      (node (ref U25) (pin 5))
      (node (ref C160) (pin 2))
      (node (ref C161) (pin 2))
      (node (ref C19) (pin 1))
      (node (ref C25) (pin 2))
      (node (ref C49) (pin 1))
      (node (ref C163) (pin 1))
      (node (ref C162) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref C54) (pin 2))
      (node (ref C45) (pin 1))
      (node (ref U3) (pin 2))
      (node (ref J2) (pin 0))
      (node (ref C40) (pin 1))
      (node (ref C55) (pin 2))
      (node (ref C60) (pin 1))
      (node (ref U25) (pin 2))
      (node (ref C57) (pin 2))
      (node (ref C63) (pin 2))
      (node (ref C65) (pin 1))
      (node (ref P20) (pin 13))
      (node (ref P20) (pin 15))
      (node (ref C78) (pin 2))
      (node (ref P5) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref FB3) (pin 2))
      (node (ref C77) (pin 2))
      (node (ref C155) (pin 2))
      (node (ref R35) (pin 2))
      (node (ref P22) (pin 18))
      (node (ref P22) (pin 10))
      (node (ref C75) (pin 2))
      (node (ref C76) (pin 1))
      (node (ref P20) (pin 19))
      (node (ref X4) (pin 7))
      (node (ref R23) (pin 2))
      (node (ref C79) (pin 2))
      (node (ref C95) (pin 2))
      (node (ref C83) (pin 2))
      (node (ref C82) (pin 2))
      (node (ref J11) (pin 2))
      (node (ref C69) (pin 2))
      (node (ref C72) (pin 2))
      (node (ref U16) (pin 2))
      (node (ref C73) (pin 1))
      (node (ref C74) (pin 1))
      (node (ref U15) (pin 26))
      (node (ref P87) (pin 1))
      (node (ref P88) (pin 1))
      (node (ref P86) (pin 1))
      (node (ref U15) (pin 25))
      (node (ref R12) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref U15) (pin 0))
      (node (ref D7) (pin 1))
      (node (ref P28) (pin 12))
      (node (ref D6) (pin 1))
      (node (ref P28) (pin 2))
      (node (ref P22) (pin 4))
      (node (ref D5) (pin 1))
      (node (ref X3) (pin 3))
      (node (ref U18) (pin 3))
      (node (ref X2) (pin 2))
      (node (ref X3) (pin 1))
      (node (ref R19) (pin 2))
      (node (ref C68) (pin 2)))
    (net (code 16) (name "Net-(J11-Pad3)")
      (node (ref J11) (pin 3)))
    (net (code 17) (name /mcu/usb/power/VBUSCTRL)
      (node (ref P20) (pin 17))
      (node (ref R7) (pin 2)))
    (net (code 18) (name I2C1_SDA)
      (node (ref P22) (pin 6))
      (node (ref U15) (pin 30))
      (node (ref U19) (pin 5))
      (node (ref R27) (pin 2)))
    (net (code 19) (name "Net-(U15-Pad10)")
      (node (ref U15) (pin 10)))
    (net (code 20) (name /mcu/usb/power/LED3)
      (node (ref R74) (pin 2))
      (node (ref U15) (pin 8))
      (node (ref P5) (pin 6)))
    (net (code 21) (name /mcu/usb/power/LED2)
      (node (ref R73) (pin 2))
      (node (ref U15) (pin 7))
      (node (ref P5) (pin 4)))
    (net (code 22) (name "Net-(U16-Pad4)")
      (node (ref U16) (pin 4)))
    (net (code 23) (name "Net-(C69-Pad1)")
      (node (ref X3) (pin 6))
      (node (ref C69) (pin 1))
      (node (ref U16) (pin 5)))
    (net (code 24) (name "Net-(X3-Pad5)")
      (node (ref X3) (pin 5)))
    (net (code 25) (name "Net-(C71-Pad2)")
      (node (ref X3) (pin 4))
      (node (ref C71) (pin 2)))
    (net (code 26) (name "Net-(C71-Pad1)")
      (node (ref C71) (pin 1))
      (node (ref R30) (pin 1))
      (node (ref U18) (pin 2))
      (node (ref L10) (pin 1)))
    (net (code 27) (name /mcu/usb/power/X3_ENABLE)
      (node (ref Q6) (pin G))
      (node (ref R21) (pin 1))
      (node (ref U15) (pin 2)))
    (net (code 28) (name CLKIN)
      (node (ref C75) (pin 1))
      (node (ref P22) (pin 2))
      (node (ref X4) (pin 8))
      (node (ref U18) (pin 4))
      (node (ref R31) (pin 2))
      (node (ref X2) (pin 3)))
    (net (code 29) (name "Net-(X2-Pad1)")
      (node (ref X2) (pin 1)))
    (net (code 30) (name /mcu/usb/power/VBUS_SENSE)
      (node (ref R12) (pin 1))
      (node (ref U15) (pin 3))
      (node (ref R10) (pin 2)))
    (net (code 31) (name "Net-(X3-Pad2)")
      (node (ref X3) (pin 2)))
    (net (code 32) (name /mcu/usb/power/VIN)
      (node (ref P20) (pin 22))
      (node (ref D10) (pin 1)))
    (net (code 33) (name "Net-(P28-Pad14)")
      (node (ref P28) (pin 14)))
    (net (code 34) (name "Net-(P28-Pad13)")
      (node (ref P28) (pin 13)))
    (net (code 35) (name "Net-(P28-Pad11)")
      (node (ref P28) (pin 11)))
    (net (code 36) (name "Net-(P28-Pad3)")
      (node (ref P28) (pin 3)))
    (net (code 37) (name "Net-(J1-Pad3)")
      (node (ref J1) (pin 3)))
    (net (code 38) (name "Net-(P22-Pad3)")
      (node (ref P22) (pin 3)))
    (net (code 39) (name "Net-(P22-Pad1)")
      (node (ref P22) (pin 1)))
    (net (code 40) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 41) (name "Net-(J1-Pad2)")
      (node (ref J1) (pin 2)))
    (net (code 42) (name "Net-(FB1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref FB1) (pin 1)))
    (net (code 43) (name TXENABLE)
      (node (ref P28) (pin 7))
      (node (ref P55) (pin 1))
      (node (ref U17) (pin 47)))
    (net (code 44) (name RXENABLE)
      (node (ref U17) (pin 48))
      (node (ref P28) (pin 8))
      (node (ref P56) (pin 1)))
    (net (code 45) (name !VAA_ENABLE)
      (node (ref R11) (pin 2))
      (node (ref Q3) (pin G))
      (node (ref P5) (pin 5))
      (node (ref U15) (pin 9)))
    (net (code 46) (name MIXER_RESETX)
      (node (ref P33) (pin 1))
      (node (ref U4) (pin 29))
      (node (ref R5) (pin 2))
      (node (ref C34) (pin 1))
      (node (ref U15) (pin 24)))
    (net (code 47) (name MIXER_ENX)
      (node (ref P28) (pin 4))
      (node (ref P32) (pin 1))
      (node (ref C35) (pin 1))
      (node (ref U4) (pin 30))
      (node (ref R6) (pin 2)))
    (net (code 48) (name MIXER_SCLK)
      (node (ref P31) (pin 1))
      (node (ref C36) (pin 1))
      (node (ref U4) (pin 31))
      (node (ref P28) (pin 5)))
    (net (code 49) (name MIXER_SDATA)
      (node (ref U4) (pin 32))
      (node (ref P27) (pin 1))
      (node (ref C37) (pin 1))
      (node (ref P28) (pin 6)))
    (net (code 50) (name CS_XCVR)
      (node (ref P28) (pin 9))
      (node (ref U17) (pin 30))
      (node (ref P53) (pin 1)))
    (net (code 51) (name XCVR_EN)
      (node (ref P28) (pin 10))
      (node (ref R41) (pin 2))
      (node (ref U17) (pin 25)))
    (net (code 52) (name "Net-(D7-Pad2)")
      (node (ref D7) (pin 2))
      (node (ref R75) (pin 1)))
    (net (code 53) (name "Net-(D5-Pad2)")
      (node (ref R73) (pin 1))
      (node (ref D5) (pin 2)))
    (net (code 54) (name "Net-(FB3-Pad1)")
      (node (ref J1) (pin 5))
      (node (ref FB3) (pin 1)))
    (net (code 55) (name VAA)
      (node (ref C87) (pin 1))
      (node (ref U17) (pin 41))
      (node (ref C6) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref C161) (pin 1))
      (node (ref C80) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref C41) (pin 1))
      (node (ref C53) (pin 1))
      (node (ref U17) (pin 7))
      (node (ref U17) (pin 19))
      (node (ref U17) (pin 1))
      (node (ref U17) (pin 13))
      (node (ref C84) (pin 1))
      (node (ref R18) (pin 2))
      (node (ref C42) (pin 1))
      (node (ref Q1) (pin S))
      (node (ref C4) (pin 1))
      (node (ref L2) (pin 2))
      (node (ref Q2) (pin S))
      (node (ref L3) (pin 2))
      (node (ref R24) (pin 2))
      (node (ref R29) (pin 1))
      (node (ref C85) (pin 1))
      (node (ref U17) (pin 39))
      (node (ref C86) (pin 1))
      (node (ref C91) (pin 1))
      (node (ref R33) (pin 2))
      (node (ref C94) (pin 1))
      (node (ref C92) (pin 1))
      (node (ref C93) (pin 1))
      (node (ref U20) (pin 1))
      (node (ref C90) (pin 1))
      (node (ref U17) (pin 28))
      (node (ref C166) (pin 1))
      (node (ref U4) (pin 22))
      (node (ref L16) (pin 1))
      (node (ref U4) (pin 5))
      (node (ref P36) (pin 1))
      (node (ref C81) (pin 1))
      (node (ref C171) (pin 1))
      (node (ref U17) (pin 46)))
    (net (code 56) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref R18) (pin 1)))
    (net (code 57) (name "Net-(D6-Pad2)")
      (node (ref D6) (pin 2))
      (node (ref R74) (pin 1)))
    (net (code 58) (name "Net-(P22-Pad13)")
      (node (ref P22) (pin 13)))
    (net (code 59) (name MIX_BYPASS)
      (node (ref U1) (pin 5))
      (node (ref U15) (pin 22))
      (node (ref U11) (pin 1))
      (node (ref C7) (pin 2))
      (node (ref P34) (pin 1))
      (node (ref C56) (pin 1)))
    (net (code 60) (name "Net-(P22-Pad19)")
      (node (ref P22) (pin 19)))
    (net (code 61) (name "Net-(P22-Pad17)")
      (node (ref P22) (pin 17)))
    (net (code 62) (name "Net-(P22-Pad16)")
      (node (ref P22) (pin 16)))
    (net (code 63) (name CLK6)
      (node (ref U19) (pin 6))
      (node (ref P22) (pin 25))
      (node (ref R85) (pin 1)))
    (net (code 64) (name "Net-(P22-Pad15)")
      (node (ref P22) (pin 15)))
    (net (code 65) (name "Net-(P22-Pad14)")
      (node (ref P22) (pin 14)))
    (net (code 66) (name "Net-(P22-Pad23)")
      (node (ref P22) (pin 23)))
    (net (code 67) (name !MIX_BYPASS)
      (node (ref C16) (pin 1))
      (node (ref U11) (pin 5))
      (node (ref P35) (pin 1))
      (node (ref U9) (pin 6))
      (node (ref C47) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref C38) (pin 2))
      (node (ref U15) (pin 14)))
    (net (code 68) (name "Net-(P22-Pad22)")
      (node (ref P22) (pin 22)))
    (net (code 69) (name "Net-(P22-Pad12)")
      (node (ref P22) (pin 12)))
    (net (code 70) (name "Net-(P22-Pad21)")
      (node (ref P22) (pin 21)))
    (net (code 71) (name "Net-(P22-Pad20)")
      (node (ref P22) (pin 20)))
    (net (code 72) (name SSP0_MOSI)
      (node (ref P22) (pin 9))
      (node (ref P40) (pin 1))
      (node (ref U17) (pin 31)))
    (net (code 73) (name SSP0_SCK)
      (node (ref P39) (pin 1))
      (node (ref U17) (pin 15))
      (node (ref P22) (pin 8)))
    (net (code 74) (name SSP0_MISO)
      (node (ref P41) (pin 1))
      (node (ref P22) (pin 7))
      (node (ref U17) (pin 29)))
    (net (code 75) (name !TX_AMP_PWR)
      (node (ref U15) (pin 20))
      (node (ref P51) (pin 1))
      (node (ref R24) (pin 1))
      (node (ref Q2) (pin G)))
    (net (code 76) (name !RX_AMP_PWR)
      (node (ref R29) (pin 2))
      (node (ref Q1) (pin G))
      (node (ref U15) (pin 16))
      (node (ref P52) (pin 1)))
    (net (code 77) (name TX_AMP)
      (node (ref P48) (pin 1))
      (node (ref U15) (pin 19))
      (node (ref C55) (pin 1))
      (node (ref C63) (pin 1))
      (node (ref U14) (pin 3))
      (node (ref U12) (pin 7)))
    (net (code 78) (name RX_AMP)
      (node (ref U12) (pin 3))
      (node (ref P49) (pin 1))
      (node (ref U14) (pin 7))
      (node (ref U15) (pin 17))
      (node (ref C60) (pin 2))
      (node (ref C66) (pin 2)))
    (net (code 79) (name TX_MIX_BP)
      (node (ref P46) (pin 1))
      (node (ref U9) (pin 3))
      (node (ref C39) (pin 2))
      (node (ref U15) (pin 13)))
    (net (code 80) (name RX_MIX_BP)
      (node (ref C40) (pin 2))
      (node (ref U9) (pin 7))
      (node (ref P47) (pin 1))
      (node (ref U15) (pin 15)))
    (net (code 81) (name LP)
      (node (ref U5) (pin 1))
      (node (ref C19) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref P45) (pin 1))
      (node (ref U6) (pin 5))
      (node (ref U15) (pin 12)))
    (net (code 82) (name HP)
      (node (ref U6) (pin 1))
      (node (ref C29) (pin 1))
      (node (ref U15) (pin 11))
      (node (ref C30) (pin 1))
      (node (ref U5) (pin 5))
      (node (ref P44) (pin 1)))
    (net (code 83) (name TX)
      (node (ref U10) (pin 5))
      (node (ref C33) (pin 1))
      (node (ref U2) (pin 5))
      (node (ref P42) (pin 1))
      (node (ref U15) (pin 23))
      (node (ref C45) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref U7) (pin 5)))
    (net (code 84) (name RX)
      (node (ref U7) (pin 1))
      (node (ref U15) (pin 21))
      (node (ref C22) (pin 2))
      (node (ref U10) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref C54) (pin 1))
      (node (ref P43) (pin 1))
      (node (ref C10) (pin 2)))
    (net (code 85) (name AMP_BYPASS)
      (node (ref P50) (pin 1))
      (node (ref C65) (pin 2))
      (node (ref U14) (pin 6))
      (node (ref C57) (pin 1))
      (node (ref U15) (pin 18))
      (node (ref U12) (pin 6)))
    (net (code 86) (name "Net-(C76-Pad2)")
      (node (ref X4) (pin 14))
      (node (ref Q7) (pin D))
      (node (ref C76) (pin 2)))
    (net (code 87) (name "Net-(P20-Pad6)")
      (node (ref P20) (pin 6)))
    (net (code 88) (name "Net-(P20-Pad14)")
      (node (ref P20) (pin 14)))
    (net (code 89) (name "Net-(P20-Pad12)")
      (node (ref P20) (pin 12)))
    (net (code 90) (name /mcu/usb/power/VBUS)
      (node (ref R10) (pin 1))
      (node (ref P20) (pin 21)))
    (net (code 91) (name "Net-(P20-Pad11)")
      (node (ref P20) (pin 11)))
    (net (code 92) (name "Net-(P20-Pad20)")
      (node (ref P20) (pin 20)))
    (net (code 93) (name "Net-(P20-Pad10)")
      (node (ref P20) (pin 10)))
    (net (code 94) (name "Net-(P20-Pad9)")
      (node (ref P20) (pin 9)))
    (net (code 95) (name "Net-(P20-Pad8)")
      (node (ref P20) (pin 8)))
    (net (code 96) (name "Net-(P20-Pad7)")
      (node (ref P20) (pin 7)))
    (net (code 97) (name "Net-(P20-Pad5)")
      (node (ref P20) (pin 5)))
    (net (code 98) (name "Net-(P20-Pad4)")
      (node (ref P20) (pin 4)))
    (net (code 99) (name "Net-(P20-Pad2)")
      (node (ref P20) (pin 2)))
    (net (code 100) (name "Net-(P20-Pad1)")
      (node (ref P20) (pin 1)))
    (net (code 101) (name "Net-(C74-Pad2)")
      (node (ref C74) (pin 2))
      (node (ref R31) (pin 1))
      (node (ref R30) (pin 2)))
    (net (code 102) (name "Net-(C73-Pad2)")
      (node (ref R23) (pin 1))
      (node (ref C73) (pin 2))
      (node (ref L10) (pin 2))
      (node (ref R22) (pin 2)))
    (net (code 103) (name "Net-(C79-Pad1)")
      (node (ref Q6) (pin D))
      (node (ref C79) (pin 1))
      (node (ref U18) (pin 5))
      (node (ref U16) (pin 3)))
    (net (code 104) (name "Net-(P20-Pad16)")
      (node (ref P20) (pin 16)))
    (net (code 105) (name RSSI)
      (node (ref P20) (pin 18))
      (node (ref P67) (pin 1))
      (node (ref U17) (pin 32)))
    (net (code 106) (name /mcu/usb/power/X4_ENABLE)
      (node (ref U15) (pin 6))
      (node (ref R32) (pin 1))
      (node (ref Q7) (pin G)))
    (net (code 107) (name "Net-(X4-Pad1)")
      (node (ref X4) (pin 1)))
    (net (code 108) (name /mcu/usb/power/!IO_INT)
      (node (ref U15) (pin 32))
      (node (ref R15) (pin 2))
      (node (ref P1) (pin 1)))
    (net (code 109) (name /mcu/usb/power/!IO_RESET)
      (node (ref P2) (pin 1))
      (node (ref R16) (pin 2))
      (node (ref U15) (pin 28)))
    (net (code 110) (name /mcu/usb/power/VBUS2_SENSE)
      (node (ref U15) (pin 4))
      (node (ref R13) (pin 2))
      (node (ref R14) (pin 1)))
    (net (code 111) (name /mcu/usb/power/X2_ENABLE)
      (node (ref R20) (pin 2))
      (node (ref R19) (pin 1))
      (node (ref Q5) (pin G))
      (node (ref R17) (pin 1))
      (node (ref U15) (pin 1)))
    (net (code 112) (name "Net-(C68-Pad1)")
      (node (ref C68) (pin 1))
      (node (ref R20) (pin 1))
      (node (ref Q5) (pin D))
      (node (ref X2) (pin 4)))
    (net (code 113) (name /mcu/usb/power/DIODE_TOWN)
      (node (ref D4) (pin 1))
      (node (ref D10) (pin 2))
      (node (ref D8) (pin 1))
      (node (ref R7) (pin 1)))
    (net (code 114) (name /mcu/usb/power/USB_SHIELD)
      (node (ref P80) (pin 2))
      (node (ref P80) (pin 1))
      (node (ref R35) (pin 1))
      (node (ref J1) (pin 0))
      (node (ref C155) (pin 1)))
    (net (code 115) (name /mcu/usb/power/BARREL_SENSE)
      (node (ref R8) (pin 2))
      (node (ref U15) (pin 5))
      (node (ref R9) (pin 1)))
    (net (code 116) (name /mcu/usb/power/BARREL)
      (node (ref R8) (pin 1))
      (node (ref D4) (pin 2))
      (node (ref J11) (pin 1)))
    (net (code 117) (name /baseband/CLK5)
      (node (ref U19) (pin 17))
      (node (ref C115) (pin 1)))
    (net (code 118) (name "Net-(FB2-Pad1)")
      (node (ref FB2) (pin 1))
      (node (ref Q3) (pin D)))
    (net (code 119) (name /baseband/XTAL2)
      (node (ref C116) (pin 1))
      (node (ref U17) (pin 17))
      (node (ref C115) (pin 2))
      (node (ref P57) (pin 1)))
    (net (code 120) (name "Net-(U19-Pad16)")
      (node (ref U19) (pin 16)))
    (net (code 121) (name "Net-(U19-Pad15)")
      (node (ref U19) (pin 15)))
    (net (code 122) (name "Net-(U19-Pad13)")
      (node (ref U19) (pin 13)))
    (net (code 123) (name "Net-(U19-Pad12)")
      (node (ref U19) (pin 12)))
    (net (code 124) (name "Net-(U19-Pad8)")
      (node (ref U19) (pin 8)))
    (net (code 125) (name "Net-(U19-Pad9)")
      (node (ref U19) (pin 9)))
    (net (code 126) (name /baseband/TXBBQ-)
      (node (ref U17) (pin 45))
      (node (ref P9) (pin 13)))
    (net (code 127) (name /baseband/TXBBQ+)
      (node (ref U17) (pin 44))
      (node (ref P9) (pin 11)))
    (net (code 128) (name /baseband/TXBBI+)
      (node (ref U17) (pin 43))
      (node (ref P9) (pin 12)))
    (net (code 129) (name /baseband/TXBBI-)
      (node (ref U17) (pin 42))
      (node (ref P9) (pin 10)))
    (net (code 130) (name /baseband/RXBBI+)
      (node (ref U17) (pin 38))
      (node (ref P9) (pin 7)))
    (net (code 131) (name /baseband/RXBBI-)
      (node (ref U17) (pin 37))
      (node (ref P9) (pin 5)))
    (net (code 132) (name /baseband/RXBBQ+)
      (node (ref U17) (pin 36))
      (node (ref P9) (pin 6)))
    (net (code 133) (name /baseband/RXBBQ-)
      (node (ref P9) (pin 4))
      (node (ref U17) (pin 35)))
    (net (code 134) (name /baseband/XB)
      (node (ref X1) (pin 1))
      (node (ref C169) (pin 2))
      (node (ref U19) (pin 2)))
    (net (code 135) (name /baseband/XA)
      (node (ref X1) (pin 3))
      (node (ref U19) (pin 1))
      (node (ref C170) (pin 2)))
    (net (code 136) (name "Net-(C106-Pad1)")
      (node (ref C106) (pin 1))
      (node (ref U17) (pin 27)))
    (net (code 137) (name "Net-(U17-Pad18)")
      (node (ref U17) (pin 18)))
    (net (code 138) (name "Net-(C104-Pad2)")
      (node (ref T4) (pin 4))
      (node (ref L8) (pin 1))
      (node (ref C104) (pin 2)))
    (net (code 139) (name "Net-(C111-Pad2)")
      (node (ref L8) (pin 2))
      (node (ref C111) (pin 2))
      (node (ref T4) (pin 3)))
    (net (code 140) (name "Net-(C104-Pad1)")
      (node (ref U17) (pin 10))
      (node (ref C104) (pin 1))
      (node (ref L9) (pin 1)))
    (net (code 141) (name "Net-(C111-Pad1)")
      (node (ref C111) (pin 1))
      (node (ref L9) (pin 2))
      (node (ref U17) (pin 11)))
    (net (code 142) (name "Net-(C99-Pad2)")
      (node (ref C99) (pin 2))
      (node (ref T3) (pin 4))
      (node (ref L6) (pin 1)))
    (net (code 143) (name "Net-(C114-Pad1)")
      (node (ref C114) (pin 1))
      (node (ref R26) (pin 2)))
    (net (code 144) (name "Net-(C114-Pad2)")
      (node (ref C114) (pin 2))
      (node (ref R25) (pin 2)))
    (net (code 145) (name /baseband/XCVR_CLKOUT)
      (node (ref U17) (pin 16))
      (node (ref P14) (pin 1)))
    (net (code 146) (name "Net-(C99-Pad1)")
      (node (ref L7) (pin 1))
      (node (ref U17) (pin 4))
      (node (ref C99) (pin 1)))
    (net (code 147) (name "Net-(C102-Pad1)")
      (node (ref C102) (pin 1))
      (node (ref U17) (pin 5))
      (node (ref L7) (pin 2)))
    (net (code 148) (name MIX_CLK)
      (node (ref C67) (pin 1))
      (node (ref U19) (pin 19)))
    (net (code 149) (name TX_IF)
      (node (ref T4) (pin 1))
      (node (ref C8) (pin 1)))
    (net (code 150) (name RX_IF)
      (node (ref T3) (pin 1))
      (node (ref C48) (pin 2)))
    (net (code 151) (name "Net-(C102-Pad2)")
      (node (ref C102) (pin 2))
      (node (ref L6) (pin 2))
      (node (ref T3) (pin 3)))
    (net (code 152) (name /baseband/CPOUT+)
      (node (ref U17) (pin 23))
      (node (ref R25) (pin 1))
      (node (ref C112) (pin 2)))
    (net (code 153) (name "Net-(C105-Pad1)")
      (node (ref P36) (pin 2))
      (node (ref FB2) (pin 2))
      (node (ref C105) (pin 1)))
    (net (code 154) (name /baseband/OEB)
      (node (ref P18) (pin 1))
      (node (ref U19) (pin 7))
      (node (ref R105) (pin 2)))
    (net (code 155) (name "Net-(C121-Pad2)")
      (node (ref U19) (pin 18))
      (node (ref C121) (pin 2))
      (node (ref L14) (pin 1)))
    (net (code 156) (name "Net-(C89-Pad1)")
      (node (ref C89) (pin 1))
      (node (ref U17) (pin 21))
      (node (ref L16) (pin 2)))
    (net (code 157) (name "Net-(C88-Pad1)")
      (node (ref C88) (pin 1))
      (node (ref L15) (pin 1))
      (node (ref U17) (pin 20)))
    (net (code 158) (name "Net-(U17-Pad9)")
      (node (ref U17) (pin 9)))
    (net (code 159) (name "Net-(U17-Pad8)")
      (node (ref U17) (pin 8)))
    (net (code 160) (name "Net-(U17-Pad6)")
      (node (ref U17) (pin 6)))
    (net (code 161) (name "Net-(U17-Pad3)")
      (node (ref U17) (pin 3)))
    (net (code 162) (name /baseband/INTR)
      (node (ref P15) (pin 1))
      (node (ref U19) (pin 3))
      (node (ref R104) (pin 2)))
    (net (code 163) (name "Net-(U17-Pad34)")
      (node (ref U17) (pin 34)))
    (net (code 164) (name "Net-(U17-Pad14)")
      (node (ref U17) (pin 14)))
    (net (code 165) (name "Net-(U17-Pad33)")
      (node (ref U17) (pin 33)))
    (net (code 166) (name "Net-(U17-Pad12)")
      (node (ref U17) (pin 12)))
    (net (code 167) (name "Net-(U17-Pad40)")
      (node (ref U17) (pin 40)))
    (net (code 168) (name /baseband/CPOUT-)
      (node (ref C112) (pin 1))
      (node (ref U17) (pin 24))
      (node (ref R26) (pin 1)))
    (net (code 169) (name "Net-(C44-Pad1)")
      (node (ref U12) (pin 1))
      (node (ref C44) (pin 1)))
    (net (code 170) (name "Net-(C160-Pad1)")
      (node (ref C162) (pin 2))
      (node (ref Q2) (pin D))
      (node (ref C160) (pin 1))
      (node (ref L12) (pin 1)))
    (net (code 171) (name /frontend/TX_AMP_IN)
      (node (ref C59) (pin 1))
      (node (ref U12) (pin 8)))
    (net (code 172) (name "Net-(C23-Pad1)")
      (node (ref C23) (pin 1))
      (node (ref U10) (pin 4)))
    (net (code 173) (name "Net-(C50-Pad1)")
      (node (ref C50) (pin 1))
      (node (ref U13) (pin 6))
      (node (ref L5) (pin 2)))
    (net (code 174) (name "Net-(C31-Pad2)")
      (node (ref C31) (pin 2))
      (node (ref U5) (pin 6)))
    (net (code 175) (name "Net-(C32-Pad1)")
      (node (ref C32) (pin 1))
      (node (ref U1) (pin 4)))
    (net (code 176) (name "Net-(C43-Pad2)")
      (node (ref C43) (pin 2))
      (node (ref U11) (pin 2)))
    (net (code 177) (name "Net-(C31-Pad1)")
      (node (ref C31) (pin 1))
      (node (ref U9) (pin 5)))
    (net (code 178) (name "Net-(C44-Pad2)")
      (node (ref U9) (pin 1))
      (node (ref C44) (pin 2)))
    (net (code 179) (name "Net-(C61-Pad1)")
      (node (ref C61) (pin 1))
      (node (ref U14) (pin 5)))
    (net (code 180) (name "Net-(C58-Pad1)")
      (node (ref U14) (pin 8))
      (node (ref C58) (pin 1)))
    (net (code 181) (name "Net-(C25-Pad1)")
      (node (ref C25) (pin 1))
      (node (ref T1) (pin 2)))
    (net (code 182) (name "Net-(P6-Pad1)")
      (node (ref P6) (pin 1))
      (node (ref U4) (pin 26)))
    (net (code 183) (name "Net-(C61-Pad2)")
      (node (ref C61) (pin 2))
      (node (ref U12) (pin 5)))
    (net (code 184) (name /frontend/TX_AMP_OUT)
      (node (ref U14) (pin 4))
      (node (ref C62) (pin 1)))
    (net (code 185) (name "Net-(C64-Pad1)")
      (node (ref U14) (pin 1))
      (node (ref C64) (pin 1)))
    (net (code 186) (name "Net-(U14-Pad2)")
      (node (ref U14) (pin 2)))
    (net (code 188) (name /frontend/RX_AMP_OUT)
      (node (ref C50) (pin 2))
      (node (ref U12) (pin 4)))
    (net (code 189) (name "Net-(L3-Pad1)")
      (node (ref L3) (pin 1))
      (node (ref T2) (pin 3))
      (node (ref U4) (pin 28))
      (node (ref L4) (pin 1)))
    (net (code 190) (name "Net-(C49-Pad2)")
      (node (ref T2) (pin 2))
      (node (ref C49) (pin 2)))
    (net (code 191) (name "Net-(C62-Pad2)")
      (node (ref C62) (pin 2))
      (node (ref L12) (pin 2))
      (node (ref U25) (pin 6)))
    (net (code 192) (name "Net-(C59-Pad2)")
      (node (ref U25) (pin 3))
      (node (ref C59) (pin 2)))
    (net (code 193) (name "Net-(C17-Pad2)")
      (node (ref U6) (pin 4))
      (node (ref C17) (pin 2)))
    (net (code 194) (name "Net-(C43-Pad1)")
      (node (ref C43) (pin 1))
      (node (ref U9) (pin 8)))
    (net (code 195) (name "Net-(C32-Pad2)")
      (node (ref C32) (pin 2))
      (node (ref U9) (pin 4)))
    (net (code 196) (name "Net-(C18-Pad1)")
      (node (ref C18) (pin 1))
      (node (ref U5) (pin 2)))
    (net (code 197) (name "Net-(C27-Pad2)")
      (node (ref U6) (pin 2))
      (node (ref C27) (pin 2)))
    (net (code 198) (name "Net-(C20-Pad2)")
      (node (ref U2) (pin 6))
      (node (ref C20) (pin 2)))
    (net (code 199) (name "Net-(C9-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref C9) (pin 2)))
    (net (code 200) (name "Net-(C51-Pad2)")
      (node (ref U10) (pin 2))
      (node (ref C51) (pin 2)))
    (net (code 201) (name "Net-(C163-Pad2)")
      (node (ref Q1) (pin D))
      (node (ref C52) (pin 1))
      (node (ref L5) (pin 1))
      (node (ref C163) (pin 2)))
    (net (code 202) (name "Net-(C28-Pad2)")
      (node (ref U7) (pin 6))
      (node (ref C28) (pin 2)))
    (net (code 203) (name "Net-(L1-Pad2)")
      (node (ref L1) (pin 2))
      (node (ref U4) (pin 24))
      (node (ref T1) (pin 3)))
    (net (code 204) (name "Net-(L1-Pad1)")
      (node (ref U4) (pin 23))
      (node (ref L1) (pin 1))
      (node (ref T1) (pin 4)))
    (net (code 205) (name "Net-(C28-Pad1)")
      (node (ref C28) (pin 1))
      (node (ref T1) (pin 1)))
    (net (code 206) (name "Net-(C21-Pad2)")
      (node (ref C21) (pin 2))
      (node (ref U7) (pin 4)))
    (net (code 207) (name "Net-(C46-Pad2)")
      (node (ref T2) (pin 1))
      (node (ref C46) (pin 2)))
    (net (code 208) (name "Net-(C8-Pad2)")
      (node (ref C8) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 209) (name "Net-(C23-Pad2)")
      (node (ref U2) (pin 4))
      (node (ref C23) (pin 2)))
    (net (code 210) (name "Net-(C58-Pad2)")
      (node (ref U13) (pin 3))
      (node (ref C58) (pin 2)))
    (net (code 211) (name "Net-(C18-Pad2)")
      (node (ref U3) (pin 1))
      (node (ref C18) (pin 2)))
    (net (code 212) (name "Net-(C14-Pad2)")
      (node (ref R3) (pin 1))
      (node (ref C14) (pin 2))
      (node (ref U4) (pin 6)))
    (net (code 213) (name "Net-(C21-Pad1)")
      (node (ref U1) (pin 2))
      (node (ref C21) (pin 1)))
    (net (code 214) (name "Net-(C51-Pad1)")
      (node (ref C51) (pin 1))
      (node (ref U11) (pin 4)))
    (net (code 215) (name "Net-(C48-Pad1)")
      (node (ref U11) (pin 6))
      (node (ref C48) (pin 1)))
    (net (code 216) (name "Net-(C46-Pad1)")
      (node (ref C46) (pin 1))
      (node (ref U10) (pin 6)))
    (net (code 217) (name "Net-(C20-Pad1)")
      (node (ref U6) (pin 6))
      (node (ref C20) (pin 1)))
    (net (code 218) (name "Net-(C26-Pad2)")
      (node (ref C26) (pin 2))
      (node (ref U5) (pin 4)))
    (net (code 219) (name "Net-(C9-Pad1)")
      (node (ref U7) (pin 2))
      (node (ref C9) (pin 1)))
    (net (code 220) (name "Net-(C17-Pad1)")
      (node (ref C17) (pin 1))
      (node (ref U3) (pin 4)))
    (net (code 221) (name "Net-(C26-Pad1)")
      (node (ref U8) (pin 3))
      (node (ref C26) (pin 1)))
    (net (code 222) (name "Net-(C27-Pad1)")
      (node (ref C27) (pin 1))
      (node (ref U8) (pin 1)))
    (net (code 223) (name "Net-(L2-Pad1)")
      (node (ref T2) (pin 4))
      (node (ref L2) (pin 1))
      (node (ref U4) (pin 27))
      (node (ref L4) (pin 2)))
    (net (code 224) (name "Net-(C12-Pad1)")
      (node (ref U4) (pin 8))
      (node (ref C12) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 225) (name "Net-(C13-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 226) (name "Net-(C15-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref C15) (pin 2)))
    (net (code 227) (name "Net-(C14-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref U4) (pin 7))
      (node (ref C15) (pin 1))
      (node (ref C14) (pin 1)))
    (net (code 228) (name "Net-(R4-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref U4) (pin 4)))
    (net (code 229) (name "Net-(P19-Pad1)")
      (node (ref U4) (pin 25))
      (node (ref P19) (pin 1)))
    (net (code 230) (name "Net-(P7-Pad1)")
      (node (ref P7) (pin 1))
      (node (ref U4) (pin 16)))
    (net (code 231) (name "Net-(P17-Pad1)")
      (node (ref U4) (pin 9))
      (node (ref P17) (pin 1)))
    (net (code 232) (name "Net-(U4-Pad1)")
      (node (ref U4) (pin 1)))
    (net (code 233) (name "Net-(C1-Pad1)")
      (node (ref U4) (pin 19))
      (node (ref C2) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref L11) (pin 1)))
    (net (code 234) (name "Net-(L13-Pad1)")
      (node (ref U20) (pin 6))
      (node (ref L13) (pin 1)))
    (net (code 235) (name "Net-(C64-Pad2)")
      (node (ref D1) (pin 2))
      (node (ref L13) (pin 2))
      (node (ref P4) (pin 1))
      (node (ref C64) (pin 2)))
    (net (code 236) (name "Net-(P3-Pad1)")
      (node (ref P3) (pin 1))
      (node (ref R33) (pin 1))
      (node (ref U20) (pin 4)))
    (net (code 237) (name /frontend/ANT_BIAS)
      (node (ref R36) (pin 1))
      (node (ref P13) (pin 1))
      (node (ref U20) (pin 3))
      (node (ref U4) (pin 15)))
    (net (code 238) (name /frontend/REF_IN)
      (node (ref P21) (pin 1))
      (node (ref C70) (pin 1))
      (node (ref U4) (pin 10))
      (node (ref C67) (pin 2)))
    (net (code 239) (name "Net-(U4-Pad20)")
      (node (ref U4) (pin 20)))
    (net (code 240) (name "Net-(U4-Pad11)")
      (node (ref U4) (pin 11)))
    (net (code 241) (name "Net-(U4-Pad21)")
      (node (ref U4) (pin 21)))
    (net (code 242) (name "Net-(U4-Pad13)")
      (node (ref U4) (pin 13)))
    (net (code 243) (name "Net-(U4-Pad14)")
      (node (ref U4) (pin 14)))
    (net (code 244) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 3)))
    (net (code 245) (name "Net-(U4-Pad2)")
      (node (ref U4) (pin 2)))
    (net (code 246) (name "Net-(U12-Pad2)")
      (node (ref U12) (pin 2)))
    (net (code 247) (name "Net-(U9-Pad2)")
      (node (ref U9) (pin 2)))
    (net (code 248) (name "Net-(U4-Pad18)")
      (node (ref U4) (pin 18)))
    (net (code 249) (name "Net-(U4-Pad17)")
      (node (ref U4) (pin 17)))))